========== StorageAdapterDescriptor ==========
	              Version: 32
	                 Size: 32
	MaximumTransferLength: 131072 (bytes)
	 MaximumPhysicalPages: 33
	        AlignmentMask: 1 (Buffers must be aligned on WORD boundaries)
	       AdapterUsesPio: True
	     AdapterScansDown: False
	      CommandQueueing: True
	  AcceleratedTransfer: True
	              BusType: BusTypeSata
	      BusMajorVersion: 2
	      BusMinorVersion: 0
dwMaxTransferLength changed [131072] -> [65536]
========== IoctlScsiGetAddress ==========
	    Length: 8
	PortNumber: 0
	    PathId: 3
	  TargetId: 0
	       Lun: 0
========== InquiryData ==========
	          DeviceType: ReadOnlyDirectAccessDevice (CD/DVD etc)
	 DeviceTypeQualifier: Active
	  DeviceTypeModifier: 0
	      RemovableMedia: Yes
	            Versions: 0
	  ResponseDataFormat: 2
	           HiSupport: Yes
	             NormACA: Yes
	       TerminateTask: No
	                AERC: No
	    AdditionalLength: 91
	       MediumChanger: No
	           MultiPort: No
	   EnclosureServices: No
	           SoftReset: No
	        CommandQueue: No
	      LinkedCommands: No
	  RelativeAddressing: No
	            VendorId: PLEXTOR 
	           ProductId: DVDR   PX-755A  
	ProductRevisionLevel: 1.08
	      VendorSpecific: 08/18/07  15:10     
========== EEPROM ==========
	      Signature: a3 03
	       VendorId: PLEXTOR 
	      ProductId: DVDR   PX-755A  
	   SerialNumber: 101973
	   Unknown[031]: ff 23 00 00 05 3b 17 01 16 54 
	            TLA: 0000
	   Unknown[045]: ff ff ff 00 ff ff 00 ff ff ff ff ff ff fa ff ff ff f1 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 00 81 12 00 fc fe 0c 44 4e fc ff 82 5b ff 0c 00 02 0b 50 0d b0 36 2d 3e a7 50 09 5a 
	   Unknown[108]: e5 00 de ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 10 10 ff ff ff ff ff ff ff a6 ff ff ff ff 00 76 10 1f fc fc 12 77 2e 02 02 02 6a 00 00 03 00 06 06 00 02 ff 04 02 44 44 11 0f ff ff ff ff ff 40 06 20 c6 ff 02 00 00 01 00 ff ff ff ff ff ee fd fe f0 02 f7 f7 f7 04 45 00 43 02 8e 04 6c 0a 00 0c 00 20 c6 31 9b 32 e5 49 ab ff ff ff ff 2f 1c 28 bd 21 fb 03 02 00 01 ee ee ff ff 19 73 01 3f ff ff 01 75 01 34 01 d5 01 78 21 b7 83 1a 
	    Silent Mode: Disable
	        SecuRec: ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
	      SpeedRead: Enable
	        Unknown: ff
	  Spindown Time: Unset
	Disc load count: 222
	   CD read time: 56:24:50
	  CD write time: 00:16:06
	  DVD read time: 08:46:26
	 DVD write time: 04:09:32
	   Unknown[050]: 00 00 00 00 ff 05 28 35 02 8d 73 04 01 02 00 19 00 9a 9a ff ff ff ff ff ff ff ff ff ff ff 00 00 00 00 00 00 00 00 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 00 05 04 
	Change BookType: for DVD+R DL
	  Auto Strategy: Unknown[ff]
	   Unknown[117]: ff ff ff ff ff ff ff ff ff ff ff ff ff 00 00 ff ff ff ff ff ff ff ff ff ff ff ff 01 01 01 03 03 04 ff ff ff 01 02 00 ff ff ff ff ff ff ff 01 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 00 01 00 01 00 00 00 00 00 23 00 00 ff ff ff ff ff 22 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff fa 05 ff ff ff ff ff ff ff ff ba 
	            Sum: fc (SpeedRead: f0 + Spindown Time: ff + BookType: fe + Auto Strategy: ff + Others)
	   Unknown[000]: ff 03 00 ff ff ff ff ff 10 7e 5e 42 00 88 ff ff 1f 0d 0a 03 ff ff 00 ff ff ff 51 55 54 18 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 8d 04 0e 2a ff ff ff ff ff ff 01 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 00 00 00 4d ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 35 38 31 37 4b 34 2d 33 36 44 53 31 30 4b 20 30 20 46 44 46 41 4c 30 34 35 4a 36 ff ff ff ff ff 46 41 52 46 58 5b ff fe ff fe 01 08 00 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff cb 47 
	   Unknown[000]: ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff fd 02 
========== GetConfiguration ==========
	    DataLength: 264
	CurrentProfile: CD-ROM
	FeatureProfileList
		DVD+R DL
		DVD+R
		DVD+RW
		DVD-R Layer Jump
		DVD-R DL
		DVD-RW Sequential
		DVD-RW
		DVD-R
		DVD-ROM
		CD-RW
		CD-R
		CD-ROM
	FeatureCore
		PhysicalInterface: ATAPI
		  DeviceBusyEvent: No
		         INQUIRY2: No
	FeatureMorphing
		Asynchronous: No
		     OCEvent: No
	FeatureRemovableMedium
		        Lockable: Yes
		DefaultToPrevent: No
		           Eject: Yes
		LoadingMechanism: Tray type loading mechanism
	FeatureRandomReadable
		        LogicalBlockSize: 2048
		                Blocking: 1
		ErrorRecoveryPagePresent: Yes
	FeatureMultiRead
		   Current: 1
		Persistent: 0
		   Version: 0
	FeatureCdRead
		          CDText: Yes
		     C2ErrorData: Yes
		DigitalAudioPlay: No
	FeaturePowerManagement
		   Current: 1
		Persistent: 1
		   Version: 0
	FeatureMicrocodeUpgrade
		M5: Yes
	FeatureTimeout
		    Group3: Yes
		UnitLength: 3332
	FeatureRealTimeStreaming
		        StreamRecording: Yes
		    WriteSpeedInGetPerf: Yes
		       WriteSpeedInMP2A: Yes
		             SetCDSpeed: Yes
		ReadBufferCapacityBlock: Yes
	FeatureLogicalUnitSerialNumber
		SerialNumber: 101973  
	VendorSpecific (FeatureCode[0xff00])
		VendorSpecificData: 01010103
	VendorSpecific (FeatureCode[0xff02])
		VendorSpecificData: 
	VendorSpecific (FeatureCode[0xff10])
		VendorSpecificData: 000a0006108a06e402c20009000a2113160d0b06058302c2
	VendorSpecific (FeatureCode[0xff11])
		VendorSpecificData: 002b000a361a2b48207615a40cfc001b000e6162569040ec2b48207615a40cfc001a00082b48207615a40cfc001500062b48207615a400140008207615a40ad205690011000e6162569040ec2b48207615a40ad2
========== SetSpeed ==========
	    RequestType: CdromSetSpeed
	      ReadSpeed: 4233KB/sec
	     WriteSpeed: 0KB/sec
	RotationControl: CdromDefaultRotation
========== ReadBufferCapacity ==========
	    TotalBufferSize: 1162KByte
	AvailableBufferSize: 1162KByte
========== ModeParmeterHeader10 ==========
	           ModeDataLength: 204
	               MediumType: 1
	  DeviceSpecificParameter: 0
	    BlockDescriptorLength: 0
========== MODE_READ_WRITE_RECOVERY_PAGE ==========
	                 PageCode: 0x01
	              PageSavable: No
	               PageLength: 10
	                   DCRBit: No
	                   PERBit: No
	                   EERBit: No
	                    RCBit: No
	                    TBBit: No
	                     ARRE: No
	                     AWRE: No
	           ReadRetryCount: 10
	          WriteRetryCount: 0
========== MODE_DISCONNECT_PAGE ==========
	                 PageCode: 0x02
	              PageSavable: No
	               PageLength: 14
	          BufferFullRatio: 4
	         BufferEmptyRatio: 240
	       BusInactivityLimit: 0
	        BusDisconnectTime: 0
	           BusConnectTime: 0
	         MaximumBurstSize: 0
	   DataTransferDisconnect: 0
========== MODE_CDROM_WRITE_PARAMETERS_PAGE ==========
	                 PageCode: 0x05
	              PageSavable: No
	               PageLength: 50
	                WriteType: 1
	                TestWrite: No
	            LinkSizeValid: No
	BufferUnderrunFreeEnabled: No
	                TrackMode: 4
	                     Copy: No
	              FixedPacket: No
	             MultiSession: 3
	            DataBlockType: 8
	                 LinkSize: 16
	      HostApplicationCode: 0
	            SessionFormat: 0
	               PacketSize: 0
	         AudioPauseLength: 150
	       MediaCatalogNumber:                 
	                     ISRC:                 
	            SubHeaderData: 0
========== VERIFY_ERROR ==========
	                 PageCode: 0x07
	                    PSBit: No
	               PageLength: 6
	                  Unknown: 0706000a0000
========== MODE_CACHING_PAGE ==========
	                 PageCode: 0x08
	              PageSavable: No
	               PageLength: 10
	         ReadDisableCache: No
	     MultiplicationFactor: No
	         WriteCacheEnable: No
	   WriteRetensionPriority: 0
	    ReadRetensionPriority: 0
	  DisablePrefetchTransfer: 0
	          MinimumPrefetch: 0
	          MaximumPrefetch: 0
	   MaximumPrefetchCeiling: 0
========== CD_DEVICE_PARAMETERS_PAGE ==========
	                 PageCode: 0x0d
	                    PSBit: No
	               PageLength: 6
	InactivityTimerMultiplier: 11
	 TheNumberOfSUnitPerMUnit: 60
	 TheNumberOfFUnitPerSUnit: 75
========== CDAUDIO_CONTROL_PAGE ==========
	                 PageCode: 0x0e
	                    PSBit: No
	               PageLength: 14
	      StopOnTrackCrossing: No
	                Immediate: Yes
	      ChannelSelection[0]: 1
	                Volume[0]: 255
	      ChannelSelection[1]: 2
	                Volume[1]: 255
	      ChannelSelection[2]: 0
	                Volume[2]: 0
	      ChannelSelection[3]: 0
	                Volume[3]: 0
========== POWER_CONDITION_PAGE ==========
	                 PageCode: 0x1a
	                    PSBit: No
	               PageLength: 10
	                  Standby: No
	                     Idle: Yes
	                IdleTimer: 1199
	             StandbyTimer: 0
========== CDVD_INACTIVITY_TIMEOUT_PAGE ==========
	                 PageCode: 0x1d
	                    PSBit: No
	               PageLength: 8
	                     SWPP: No
	                     DISP: No
	   GroupOneMinimumTimeout: 0
	   GroupTwoMinimumTimeout: 0
========== CDVD Capabilities & Mechanism Status Page ==========
	                 PageCode: 0x2a
	                    PSBit: No
	               PageLength: 50
	                  CDRRead: Yes
	                  CDERead: Yes
	                  Method2: Yes
	               DVDROMRead: Yes
	                 DVDRRead: Yes
	               DVDRAMRead: No
	                 CDRWrite: Yes
	                 CDEWrite: Yes
	                TestWrite: Yes
	                DVDRWrite: Yes
	              DVDRAMWrite: No
	                AudioPlay: Yes
	                Composite: Yes
	           DigitalPortOne: No
	           DigitalPortTwo: No
	               Mode2Form1: Yes
	               Mode2Form2: Yes
	             MultiSession: Yes
	       BufferUnderrunFree: Yes
	                     CDDA: Yes
	             CDDAAccurate: Yes
	              RWSupported: Yes
	          RWDeinterleaved: Yes
	               C2Pointers: Yes
	                     ISRC: Yes
	                      UPC: Yes
	       ReadBarCodeCapable: No
	                     Lock: Yes
	                LockState: No
	            PreventJumper: No
	                    Eject: Yes
	     LoadingMechanismType: tray
	           SeparateVolume: Yes
	      SeperateChannelMute: Yes
	      SupportsDiskPresent: No
	          SWSlotSelection: No
	        SideChangeCapable: No
	       RWInLeadInReadable: Yes
	         ReadSpeedMaximum: 8467KB/sec (48x)
	       NumberVolumeLevels: 256
	               BufferSize: 2048
	         ReadSpeedCurrent: 4234KB/sec (24x)
	                      BCK: No
	                      RCK: No
	                     LSBF: No
	                   Length: 0
	        WriteSpeedMaximum: 8467KB/sec (48x)
	        WriteSpeedCurrent: 8467KB/sec (48x)
	   CopyManagementRevision: 0
========== Check main + c2 + sub ==========
========== LBA[000000, 0000000]: C2 error ==========
       +0 +1 +2 +3 +4 +5 +6 +7
0000 : 00 00 00 00 00 00 00 00
0008 : 00 00 00 00 00 00 00 00
0010 : 00 00 00 00 00 00 00 00
0018 : 00 00 00 00 00 00 00 00
0020 : 00 00 00 00 00 00 00 00
0028 : 00 00 00 00 00 00 00 00
0030 : 00 00 00 00 00 00 00 00
0038 : 00 00 00 00 00 00 00 00
0040 : 00 00 00 00 00 00 00 00
0048 : 00 00 00 00 00 00 00 00
0050 : 00 00 00 00 00 00 00 00
0058 : 00 00 00 00 00 00 00 00
0060 : 00 00 00 00 00 00 00 00
0068 : 00 00 00 00 00 00 00 00
0070 : 00 00 00 00 00 00 00 00
0078 : 00 00 00 00 00 00 00 00
0080 : 00 00 00 00 00 00 00 00
0088 : 00 00 00 00 00 00 00 00
0090 : 00 00 00 00 00 00 00 00
0098 : 00 00 00 00 00 00 00 00
00A0 : 00 00 00 00 00 00 00 00
00A8 : 00 00 00 00 00 00 00 00
00B0 : 00 00 00 00 00 00 00 00
00B8 : 00 00 00 00 00 00 00 00
00C0 : 00 00 00 00 00 00 00 00
00C8 : 00 00 00 00 00 00 00 00
00D0 : 00 00 00 00 00 00 00 00
00D8 : 00 00 00 00 00 00 00 00
00E0 : 00 00 00 00 00 00 00 00
00E8 : 00 00 00 00 00 00 00 00
00F0 : 00 00 00 00 00 00 00 00
00F8 : 00 00 00 00 00 00 00 00
0100 : 00 00 00 00 00 00 00 00
0108 : 00 00 00 00 00 00 00 00
0110 : 00 00 00 00 00 00 00 00
0118 : 00 00 00 00 00 00 00 00
0120 : 00 00 00 00 00 00 80 C0
========== LBA[000000, 0000000]: Sub Channel(Raw) ==========
       +0 +1 +2 +3 +4 +5 +6 +7  +8 +9 +A +B +C +D +E +F
0000 : 80 C0 80 80 80 80 80 C0  80 80 80 80 80 80 80 C0
0010 : 80 80 80 80 80 80 80 C0  80 80 80 80 80 80 80 80
0020 : 80 80 80 80 80 80 80 80  80 80 80 80 80 80 80 80
0030 : 80 80 80 80 80 80 80 80  80 80 80 80 80 80 80 80
0040 : 80 80 80 80 80 80 C0 80  80 80 80 80 80 80 80 80
0050 : 80 80 C0 80 C0 80 80 80  80 80 C0 C0 80 80 C0 80
========== Check main + sub + c2 ==========
========== LBA[000000, 0000000]: Sub Channel(Raw) ==========
       +0 +1 +2 +3 +4 +5 +6 +7  +8 +9 +A +B +C +D +E +F
0000 : 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00
0010 : 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00
0020 : 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00
0030 : 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00
0040 : 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00
0050 : 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00
========== LBA[000000, 0000000]: C2 error ==========
       +0 +1 +2 +3 +4 +5 +6 +7
0000 : 00 00 00 00 00 00 00 00
0008 : 00 00 00 00 00 00 00 00
0010 : 00 00 00 00 00 00 00 00
0018 : 00 00 00 00 00 00 00 00
0020 : 00 00 00 00 00 00 00 00
0028 : 00 00 00 00 00 00 00 00
0030 : 00 00 00 00 00 00 00 00
0038 : 00 00 00 00 00 00 00 00
0040 : 00 00 00 00 00 00 00 00
0048 : 00 00 00 00 00 00 00 00
0050 : 00 00 00 00 00 00 00 00
0058 : 00 00 00 00 00 00 00 00
0060 : 00 00 00 00 00 00 00 00
0068 : 00 00 00 00 00 00 00 00
0070 : 00 00 00 00 00 00 00 00
0078 : 00 00 00 00 00 00 00 00
0080 : 00 00 00 00 00 00 00 00
0088 : 00 00 00 00 00 00 00 00
0090 : 00 00 00 00 00 00 00 00
0098 : 00 00 00 00 00 00 00 00
00A0 : 00 00 00 00 00 00 00 00
00A8 : 00 00 00 00 00 00 00 00
00B0 : 00 00 00 00 00 00 00 00
00B8 : 00 00 00 00 00 00 00 00
00C0 : 00 00 00 00 00 00 80 C0
00C8 : 80 80 80 80 80 C0 80 80
00D0 : 80 80 80 80 80 C0 80 80
00D8 : 80 80 80 80 80 C0 80 80
00E0 : 80 80 80 80 80 80 80 80
00E8 : 80 80 80 80 80 80 80 80
00F0 : 80 80 80 80 80 80 80 80
00F8 : 80 80 80 80 80 80 80 80
0100 : 80 80 80 80 80 80 80 80
0108 : 80 80 80 80 C0 80 80 80
0110 : 80 80 80 80 80 80 80 80
0118 : C0 80 C0 80 80 80 80 80
0120 : C0 C0 80 80 C0 80 00 00
	Byte order of this drive is main + c2 + sub
This drive supports [OpCode: 0xd8, SubCode: 0]
This drive supports [OpCode: 0xd8, SubCode: 1]
This drive supports [OpCode: 0xd8, SubCode: 2]
This drive supports [OpCode: 0xd8, SubCode: 8]
Checking reading lead-out -> OK
