[dialog]
   caption= "日本語ＤＯＳアプリケーションの登録"

[macro]

[pif_default]
; デフォルトは次のとおりです。
;
; ほかのオプションは参照用です。
; ( (or) はラジオ ボタン グループに対応するエントリを意味します)
;
convmem        = 128,640      ; ##,## (必要,上限)
emsmem         = 0,1024       ; ##,## (必要,上限)
xmsmem         = 0,1024       ; ##,## (必要,上限)
dispusage      = fs           ; (or) win
execflags      =              ; bgd, exc
multaskopt     = 20,100       ; ##,## (Bgd Pri, Fgd Pri)
procmemflags   = dit,hma,eml  ; eml,xml,lam
dispoptvideo   = hgr          ; (or) txt,lgr
dispoptports   = hgr          ; txt,lgr
dispflags      = emt          ; rvm
otheroptions   = afp          ; cwa,ata,aes,ces,psc,aps,asp,aen
execmode       =              ; nmode,hmode,win (モード指定)
videomemcopy   = txt          ; gra
graphcopyplane =              ; p1,p2,p3,p4
nonmonitorport =              ; c8,c16,grw,tgdc,ggdc,frw
emsmode        = spg          ; lpg
rshandshake    =              ; rscs,xon,erdr

[dos_pifs]
123.exe     = 123r23j   ,"Lotus 1-2-3 R2.3J"        ,appsicon.dll ,29 ,enh_123r23j   ,bat_123r23j  ,dev_matutake
al.exe      = a_leter   ,"アシストレター"           ,appsicon.dll , 1 ,enh_a_leter   ,bat_a_leter
aw.exe      = a_word    ,"アシストワード"           ,appsicon.dll , 2 ,enh_a_word    ,bat_a_word
crd.exe     = card3     ,"The CARD 3+"              ,appsicon.dll , 3 ,enh_card3     ,bat_card3    ,dev_vjeb25
dcad.exe    = dynacad   ,"DynaCAD"                  ,appsicon.dll ,17 ,enh_dynacad   ,bat_dynacad  ,dev_dynacad
dease.bat   = dataease  ,"DATAEASE"                 ,appsicon.dll ,15 ,enh_dataease  ,bat_dataease ,dev_dataease
f1ld.exe    = f1dbox    ,"F-1 DATABOX V 2.5"        ,appsicon.dll ,28 ,enh_f1dbox    ,bat_f1dbox   ,dev_f1dbox
fe.exe      = final     ,"Screen Editor Final"      ,appsicon.dll , 7 ,enh_final     ,bat_final
gninja.exe  = ninja4    ,"Ninja(忍者)4"             ,appsicon.dll ,10 , enh_ninja4   ,bat_ninja4   ,dev_katana4
dv.bat      = diva      ,"DIVA"                     ,appsicon.dll ,16 ,enh_diva      ,bat_diva     ,dev_diva
hana.com    = hana22    ,"花子 Ver2.2"              ,appsicon.dll ,12 , enh_hana22   ,bat_hana22   ,dev_atok7l
iris.exe    = iris40    ,"Let'sｱｲﾘｽ4.0"             ,appsicon.dll ,22 , enh_iris40   ,bat_iris40
jg.exe      = jg30      ,"JG Ver 3.0"               ,appsicon.dll ,31 , enh_jg30     ,bat_jg30     ,dev_vjeb30
jdash.com   = jdash     ,"一太郎 dash"              ,appsicon.dll ,13 , enh_jdash    ,bat_jdash    ,dev_jdash
jxw.com     = jxw43     ,"一太郎 Ver4.3"            ,appsicon.dll ,14 , enh_jxw43    ,bat_jxw43    ,dev_atok7l
kid98.exe   = kid30     ,"Z's STAFF KID 98 Ver 3.0" ,appsicon.dll ,32 , enh_kid30    ,bat_kid30    ,dev_kid30
kiri.exe    = kiri4     ,"桐 Ver4 （松茸Ver3.5使用）",appsicon.dll ,34 , enh_kiri4    ,bat_kiri4    ,dev_kiri4
kiri.exe    = kiri4e    ,"桐 Ver4 （松茸Ver3.7使用）",appsicon.dll ,34 , enh_kiri4e   ,bat_kiri4e   ,dev_mttk3
kword.com   = k_word    ,"Katana(刀) Word"          ,appsicon.dll , 9 , enh_k_word   ,bat_k_word   ,dev_katana4
m2020.com   = a_calc    ,"アシストカルク"           ,appsicon.dll , 0 ,enh_a_calc    ,bat_a_calc
matu.com    = matu6     ,"松 Ver6"                  ,appsicon.dll ,33 ,enh_matu6     ,bat_matu6    ,dev_mttk3
mifes.exe   = mifes     ,"MIFES"                    ,appsicon.dll ,27 ,enh_mifes     ,bat_mifes
ob3.exe     = obanto_3  ,"三代目大番頭"             ,appsicon.dll ,26 ,enh_obanto_3  ,bat_obanto_3
pcastart.exe= pca_bps   ,"PCA SOFT"                 ,appsicon.dll ,24 ,enh_pca_bps   ,bat_pca_bps  ,dev_pca_bps
pcom.exe    = pcom_alp  ,"PCOM αシリーズ"          ,appsicon.dll ,21 ,enh_pcom_alp  ,bat_pcom_alp
pharapc.exe = pharaoh   ,"ファラオ"                 ,appsicon.dll , 5 ,enh_pharaoh   ,bat_pharaoh
phutypc.exe = pharauty  ,"ファラオ ユーティリティ"  ,appsicon.dll , 6 ,enh_pharauty  ,bat_pharauty
pp.exe      = pagepro3  ,"PagePro(DOS Ver3.xx使用)" ,appsicon.dll , 4 ,enh_pagepro3  ,bat_pagepro3 ,dev_pagepro3
pp.exe      = pagepro5  ,"PagePro(DOS Ver5.xx使用)" ,appsicon.dll , 4 ,enh_pagepro5  ,bat_pagepro5
rbase.exe   = rbase31   ,"R:BASE PRO Ver.3.1"       ,appsicon.dll ,23 ,enh_rbase31   ,bat_rbase31
topa.bat    = topaknd   ,"TOP 商人"                 ,appsicon.dll , 8 ,enh_topaknd   ,bat_topaknd  ,dev_top2
top2.exe    = top2      ,"TOP2シリーズ"             ,appsicon.dll , 8 ,enh_top2      ,bat_top2     ,dev_top2
vp.exe      = vjepen3   ,"VJE-Pen Ver 3.0"          ,appsicon.dll ,20 ,enh_vjepen3   ,bat_vjepen3  ,dev_vjepen3
works.exe   = works25   ,"Microsoft Works Ver.2.5"  ,appsicon.dll ,25 ,enh_works25   ,bat_works25  ,dev_works25
wp.exe      = wperfect  ,"WordPerfect 5.1J"         ,appsicon.dll ,19 ,enh_wperfect  ,bat_wperfect ,dev_wperfect
ws.exe      = ws70      ,"WordStar for DOS 7.0"     ,appsicon.dll ,30 ,enh_ws70      ,bat_ws70
y3menu.exe  = yayoi_3   ,"弥生3シリーズ"            ,appsicon.dll ,18 ,enh_yayoi_3   ,bat_yayoi_3  ,dev_yayoi_3
zero.exe    = zero_2    ,"ZERO2 (DOS3.3x)"          ,appsicon.dll ,11 , enh_zero_2   ,bat_zero_2   ,dev_katana4
zero.exe    = zero_2d5  ,"ZERO2 (DOS5.0x)"          ,appsicon.dll ,11 , enh_zero_2d5 ,bat_zero_2d5 ,dev_ktn4d5

[fep_default]
default     =

[feps]
;ev_egb98   = egb98    ,"ＥＧ−Ｂｒｉｄｇｅ"
dev_atok7   = atok7    ,"ＡＴＯＫ　７"
dev_atok7l  = atok7L   ,"ＡＴＯＫ　７"
dev_katana4 = katana4  ,"Ｋａｔａｎａ(刀) Ver 4"
dev_vjeb25  = vjeb25   ,"ＶＪＥ−β Ver 2.5"
dev_vjeb30  = vjeb30   ,"ＶＪＥ−β Ver 3.0"
dev_matutake= matutake ,"松茸 Ver2.11"
dev_mttk3   = mttk3    ,"松茸 Ver3"

[dos_files]
atok7a.sys  = "ATOK7 ドライバ",         dev_atok7,dev_atok7l,dev_jdash
atok7b.sys  = "ATOK7 ドライバ",         dev_atok7,dev_atok7l,dev_jdash
atok7d.dic  = "ATOK7 辞書",             dev_jdash
;atok7.dic   = "ATOK7 辞書",             dev_atok7
atok7l.dic  = "ATOK7 辞書",             dev_atok7l
egb98.sys   = "EG-Bridge ドライバ",     dev_a_leter
egb98if.sys = "EG-Bridge ドライバ",     dev_a_leter
jfgaij.ufo  = "ATOK7 外字辞書",         dev_atok7,dev_atok7l,dev_jdash
jj2.sys     = "JJ Ver 1.25",            dev_f1dbox
ktn.dic     = "Katana(刀) 辞書",        dev_katana4
ktn4.sys    = "Katana(刀) ドライバ",    dev_katana4
ktn4c.sys   = "Katana(刀) ドライバ",    dev_katana4
mcode.drv   = "松茸 Ver3 ドライバ",     dev_mttk3
mouse.sys   = "マウス ドライバ",        dev_matutake,dev_dynacad,dev_pagepro3
mttk2.drv   = "松茸 ドライバ",          dev_matutake
mttk3.drv   = "松茸 Ver3 ドライバ",     dev_kiri4
mttk3a.drv  = "松茸 Ver3 ドライバ",     dev_mttk3
mttk3b.drv  = "松茸 Ver3 ドライバ",     dev_mttk3
print.sys   = "PRINT.SYS",              dev_pca_bps
prun.exe    = "PCA SOFT Loader",        bat_pca_bps
rsdrv.sys   = "RSドライバ",             dev_f1dbox, dev_kid30,dev_dynacad
usr.dic    = "Katana(刀) 辞書",        dev_katana4
vje.sys     = "VJE-Σ Ver1.20 ドライバ",dev_kid30
vjeb.dic    = "VJE-β 辞書",            dev_vjeb25, dev_yayoi_3, dev_top2,dev_dynacad
vjeb.drv    = "VJE-β Ver1.20R ドライバ", bat_topaknd, bat_top2,dev_top2, bat_pca_bps, dev_pca_bps
vjeb.drv    = "VJE-β Ver2.1 ドライバ", dev_dynacad,bat_dynacad
vjeb.drv    = "VJE-β Ver2.5 ドライバ", dev_vjeb25, dev_yayoi_3
vjeb.drv    = "VJE-β Ver3.0 ドライバ", dev_vjeb30,bat_jg30, dev_vjepen3, bat_vjepen3, dev_works25, bat_works25, dev_diva, bat_diva, bat_dataease, dev_dataease
wpfep.sys   = "WPFEP Ver 1.00",         dev_wperfect
wpkb.sys    = "WPFEP Ver 1.00",         dev_wperfect

;**************************************** [enh_<pifname>]セクション
[enh_card3]
convmem = 420,640

[enh_a_calc]
convmem = 640,640
execflags = exc
videomemcopy = gra
graphcopyplane = p1,p2,p3,p4

[enh_a_leter]
convmem = 640,640
dispoptvideo = txt
dispoptports = txt
videomemcopy = gra
graphcopyplane = p1,p2,p3,p4

[enh_a_word]
convmem = 640,640
execflags = exc
videomemcopy = gra
graphcopyplane = p1,p2,p3,p4

[enh_pagepro3]
convmem = 410,640
execmode  = nmode

[enh_pagepro5]
convmem = 410,640
execmode  = nmode

[enh_pharaoh]
execflags = exc

[enh_pharauty]
execflags = exc

[enh_final]
convmem = 384,640
execflags = bgd
multaskopt   = 50,100
dispoptvideo = txt
dispoptports = txt

[enh_topaknd]
convmem = 640,640
execflags = exc
videomemcopy = gra
graphcopyplane = p1,p2,p3,p4

[enh_top2]
convmem = 640,640
execflags = exc
videomemcopy = gra
graphcopyplane = p1,p2,p3,p4

[enh_k_word]
convmem = 384,640
execflags = exc
procmemflags = hma,eml

[enh_zero_2]
convmem = 450,640
execflags = exc
emsmem  = 64,2048
procmemflags = hma,eml

[enh_zero_2d5]
convmem = 450,640
execflags = exc
emsmem  = 64,2048
procmemflags = hma,eml

[enh_ninja4]
convmem = 256,640
execflags = exc
procmemflags = hma,eml

[enh_obanto_3]
execmode = nmode
dispoptvideo = txt
dispoptports = txt

[enh_up2sys]
convmem = 480,-1
multaskopt   = 100,100
emsmem  =  512,-1
xmsmem  = 0,0
rshandshake = xon
videomemcopy = gra
graphcopyplane = p1,p2,p3

[enh_hana22]
convmem = 480,640
xmsmem  = 0,0
multaskopt   = 5,100
videomemcopy = gra
graphcopyplane = p1,p2,p3,p4

[enh_jdash]
convmem = 480,640
xmsmem  = 0,0
multaskopt   = 5,100

[enh_jxw43]
convmem = 480,640
xmsmem  = 0,0
multaskopt   = 5,100

[enh_jg30]
convmem = 450,640
execmode = nmode
videomemcopy = gra
graphcopyplane = p1,p2,p3,p4

[enh_kid30]
convmem = 430,640
execmode = nmode
videomemcopy = gra
graphcopyplane = p1,p2,p3,p4

[enh_yayoi_3]
convmem = 410,640
otheroptions = psc

[enh_wperfect]
convmem = 420,640
multaskopt   = 50,100

[enh_works25]

[enh_pcom_alp]
convmem = 384,640
execflags = exc
execmode = nmode
dispoptvideo = txt
dispoptports = txt

[enh_iris40]

[enh_vjepen3]
dispoptvideo = txt
dispoptports = txt

[enh_pca_bps]
convmem = 440,640
execmode = nmode
dispoptvideo = txt
dispoptports = txt

[enh_rbase31]
convmem = 480,640
execflags = exc
dispoptvideo = txt
dispoptports = txt
emsmem  = 0,2048
xmsmem  = 1024,2048
videomemcopy = gra
graphcopyplane = p1,p2,p3,p4

[enh_mifes]

[enh_matu6]
convmem = 480,640
emsmem  =  512,2048
xmsmem  = 0,1024
rshandshake = rscs

[enh_kiri4]
convmem = 480,640
emsmem  =  512,2048
xmsmem  = 0,1024
rshandshake = rscs

[enh_kiri4e]
convmem = 480,640
emsmem  =  512,2048
xmsmem  = 0,1024
rshandshake = rscs

[enh_f1dbox]
convmem = 400,640
execflags = exc
rshandshake = xon
emsmem  = 0,1024

[enh_123r23j]
convmem = 0,640
execflags = exc
multaskopt   = 50,100
emsmem  = 0,2048
dispoptvideo = txt
dispoptports = txt

[enh_ws70]
convmem = 512,640
multaskopt   = 50,100
procmemflags = dit,eml
xmsmem  = 0,0

[enh_diva]
convmem = 480,-1
multaskopt   =100,100
emsmem  =  512,-1
xmsmem  = 0,0
execflags = exc
rshandshake = xon
videomemcopy = gra
graphcopyplane = p1,p2,p3
nonmonitorport = frw

[enh_dataease]
convmem = 384,640
execflags = exc
multaskopt   =100,100
emsmem  = 0,128
xmsmem  = 64,64
execflags = exc
videomemcopy = gra
graphcopyplane = p1,p2,p3,p4
nonmonitorport = frw

[enh_dynacad]
convmem = 640,640
execmode = nmode
emsmem  = 0,128
xmsmem  = 0,0
execflags = exc
rshandshake = xon
videomemcopy = gra
graphcopyplane = p1,p2,p3,p4
nonmonitorport = frw

;**************************************** [bat_<pifname>]セクション
[bat_card3]
adddrv @{devfile}
@{exedrv}
cd @{exedir}
@6{exefile}
deldrv

[bat_a_calc]
adddrv @{devfile}
set 2020EMEM=0
@{exedrv}
cd @{exedir}
@6{exefile}
cd \
set 2020EMEM=
deldrv

[bat_a_leter]
adddrv @{devfile}
@{exedrv}
cd @{exedir}
@6{exefile}
cd \
deldrv

[bat_a_word]
adddrv @{devfile}
@{exedrv}
cd @{exedir}
@6{exefile}
cd \
deldrv

[bat_pagepro3]
adddrv @{devfile}
@{exedrv}
cd @{exedir}
@6{exefile}
deldrv

[bat_pagepro5]
mouse
adddrv @{devfile}
@{exedrv}
cd @{exedir}
@6{exefile}
deldrv

[bat_pharaoh]
echo off
@{exedrv}
cd @{exedir}
@6{exefile}

[bat_pharauty]
echo off
@{exedrv}
cd @{exedir}
:loop
    @6{exefile}
    if errorlevel 6 goto drv_f
    if errorlevel 5 goto drv_e
    if errorlevel 4 goto drv_d
    if errorlevel 3 goto drv_c
    if errorlevel 2 goto drv_b
    if errorlevel 1 goto drv_a
    goto end
:drv_a
    format a:
    goto loop
:drv_b
    format b:
    goto loop
:drv_c
    format c:
    goto loop
:drv_d
    format d:
    goto loop
:drv_e
    format e:
    goto loop
:drv_f
    format f:
    goto loop
:end
echo on

[bat_final]
echo off
adddrv @{devfile}
@{exedrv}
cd @{exedir}
@6{exefile}
deldrv

[bat_topaknd]
@3{vjeb.drv}
cd @1{vjeb.drv}
adddrv @{devfile}
@{exedrv}
cd @{exedir}
command /c @{exefile}
deldrv

[bat_top2]
@3{vjeb.drv}
cd @1{vjeb.drv}
adddrv @{devfile}
@{exedrv}
cd @{exedir}
@6{exefile}
deldrv

[bat_k_word]
cls
adddrv @{devfile}
@{exedrv}
cd @{exedir}
title
@6{exefile}
deldrv

[bat_zero_2]
cls
adddrv @{devfile}
@{exedrv}
cd @{exedir}
title
@6{exefile}
deldrv

[bat_zero_2d5]
cls
adddrv @{devfile}
@{exedrv}
cd @{exedir}
title
@6{exefile}
deldrv

[bat_ninja4]
cls
adddrv @{devfile}
@{exedrv}
cd @{exedir}
@6{exefile}   @{exedir}
deldrv

[bat_obanto_3]
echo off
rem ***********************************
rem          ＦＥＰの組み込み
rem ***********************************
adddrv @{devfile}

rem ***********************************
rem          大番頭の起動
rem ***********************************
@{exedrv}
cd @{exedir}
cls
@6{exefile} @1{exefile}
cd \
@{exedrv}
cls

rem ***********************************
rem          ＦＥＰの取り外し
rem ***********************************
deldrv > NUL

[bat_up2sys]
echo off
adddrv @{devfile}
@{exedrv}
cls
echo Dynaware Window (C)	Copyright 1989 by Dynaware Corp.
cd @{exedir}

mmems -m
if errorlevel 1 goto BANK
echo MMEMS (ＥＭＳ用メモリマネージャ) が組み込まれました
goto FEP

:BANK
isxa
if errorlevel 1 goto XABANK
mmiobank -m
if errorlevel 1 goto MEM
echo MMIOBANK (IO-BANK用メモリマネージャ) が組み込まれました
goto FEP

:XABANK
mmxabank -m
if errorlevel 1 goto MEM
echo MMXABANK (XA-BANK用メモリマネージャ) が組み込まれました
goto FEP

:MEM
mm -m
echo MM (メインメモリ用メモリマネージャ) が組み込まれました

:FEP
isvje
if errorlevel 1 goto VJE
isxa 
if errorlevel 1 goto XANOVJE
dwd2f %1 %2 %3 %4 %5 %6 %7 %8 %9 /dd B:\
goto END

:XANOVJE
dwd2xaf %1 %2 %3 %4 %5 %6 %7 %8 %9 /dd B:\
goto END

:VJE
isxa
if errorlevel 1 goto XAVJE
dwd2v %1 %2 %3 %4 %5 %6 %7 %8 %9 /dd B:\
goto END

:XAVJE
dwd2xav %1 %2 %3 %4 %5 %6 %7 %8 %9 /dd B:\ 
:END
mm -r
cls2
cd \
deldrv

[bat_hana22]
echo off
rem Add ATOK7
set path=@{exedir}\..\jsw;%path%
adddrv @{devfile}

rem Change current drive
@{exedrv}
rem Change current directory
cd @{exedir}

rem Execute
@6{exefile}

rem Delete added character device
deldrv

[bat_jdash]
echo off
rem Add ATOK7
set path=@{exedir}\..\jsw;%path%
adddrv @{devfile}

rem Change current drive
@{exedrv}
rem Change current directory
cd @{exedir}

rem Execute
@6{exefile}

rem Delete added character device
deldrv

[bat_jxw43]
echo off
rem Add ATOK7
set path=@{exedir}\..\jsw;%path%
adddrv @{devfile}

rem Change current drive
@{exedrv}
rem Change current directory
cd @{exedir}

rem Execute
@6{exefile}

rem Delete added character device
deldrv

[bat_jg30]
@3{vjeb.drv}
cd @1{vjeb.drv}
adddrv @{devfile}
@{exedrv}
cd @{exedir}
@6{exefile}
deldrv

[bat_kid30]
@{exedrv}
cd @{exedir}
adddrv @{devfile}
@6{exefile}
deldrv

[bat_yayoi_3]
adddrv @{devfile}
@{exedrv}
cd @{exedir}
@6{exefile}
deldrv

[bat_wperfect]
@{exedrv}
cd @{exedir}
adddrv @{devfile}
@6{exefile}
deldrv

[bat_pcom_alp]
ECHO OFF
@{exedrv}
cd @{exedir}
:START
CLS
ECHO               ---------------------------------------       
ECHO                 ただ今、 ＰＣＯＭを読み込んでいます
ECHO 　  　　　　  ---------------------------------------
@6{exefile} -M
      IF ERRORLEVEL 4 GOTO MENU1
      IF ERRORLEVEL 3 GOTO MNP1
      IF ERRORLEVEL 2 GOTO MNP2
      IF ERRORLEVEL 1 GOTO FMENT1
GOTO EX
:MENU1
CLS
ECHO             --------------------------------------------------
ECHO                ただ今、メニュープログラムを読み込んでいます
ECHO             --------------------------------------------------
PMENU
GOTO START
:MNP1
CLS
TYPE MNP1.DOC
PAUSE
CLS
TYPE MNP2.DOC
PAUSE
PCOM -1200 -NOWD -CD MNP\ -NOMSG -AUTO
GOTO START
:MNP2
CLS
TYPE MNPN1.DOC
PAUSE
CLS
TYPE MNPN2.DOC
PAUSE
PCOM -1200 -NOWD -CD MNPN\ -NOMSG -AUTO
GOTO START
:FMENT1
CLS
ECHO        -----------------------------------------------------------
ECHO          ただ今、 ファイル作成・修正プログラムを読み込んでいます
ECHO        -----------------------------------------------------------
FMENT
GOTO START
:EX

[bat_iris40]
@{exedrv}
cd @{exedir}
adddrv @{devfile}
@6{exefile}
deldrv

[bat_vjepen3]
@3{vjeb.drv}
cd @1{vjeb.drv}
adddrv @{devfile}
@{exedrv}
cd @{exedir}
echo [VJE-Pen Ver.3.0] Loading ････
vps -! -a
@6{exefile} -#" VJE-Pen Ver.3.0 " %1 %2 %3 %4 %5
deldrv

[bat_pca_bps]
@3{vjeb.drv}
cd @1{vjeb.drv}
adddrv @{devfile}
@{exedrv}
cd @{exedir}
@{prun.exe} @6{exefile}
deldrv

[bat_rbase31]
@{exedrv}
cd @{exedir}
adddrv @{devfile}
@6{exefile}
deldrv

[bat_mifes]
@{exedrv}
cd @{exedir}
adddrv @{devfile}
@6{exefile}
deldrv

[bat_works25]
echo off
@3{vjeb.drv}
cd @1{vjeb.drv}
adddrv @{devfile}
@{exedrv}
cd @{exedir}
	if exist mskn.exe mskn  
	if not exist mouse.com goto nomouse
	mouse
	if errorlevel 1 goto nomouse
:mouse
	@6{exefile} %1 %2 %3 %4 %5 %6 %7 %8 %9
	mouse off
	goto end
:nomouse
	@6{exefile} %1 %2 %3 %4 %5 %6 %7 %8 %9
	goto end
:end
	if exist mskn.exe mskn off
	deldrv

[bat_f1dbox]
echo off
cls
@{exedrv}
cd @{exedir}
adddrv @{devfile}
@6{exefile} %1
deldrv

[bat_123r22j]
cls
@{exedrv}
cd @{exedir}
adddrv @{devfile}
@6{exefile}
cd \
deldrv

[bat_123r23j]
cls
@{exedrv}
cd @{exedir}
mousel
adddrv @{devfile}
@6{exefile}
cd \
deldrv

[bat_ws70]
@{exedrv}
cd @{exedir}
@6{exefile}

[bat_diva]
echo off
@3{vjeb.drv}
cd @1{vjeb.drv}
adddrv @{devfile}
@{exedrv}
cd @{exedir}
command /c @{exefile}
deldrv

[bat_dynacad]
echo off

rem -----for Windows
@3{vjeb.drv}
cd @1{vjeb.drv}
adddrv @{devfile}

@{exedrv}
cls
speed R0 9600 B7 PE S1 XON
cd @{exedir}
dcad %1 %2 %3 %4 %5
cd \

rem -----for Windows
deldrv

[bat_dataease]
echo off
@3{vjeb.drv}
cd @1{vjeb.drv}
adddrv @{devfile}
@{exedrv}
cd @{exedir}
command /c @{exefile}
deldrv
echo on

[bat_matu6]
echo off
rem set path=a:\matuv6;%path%;

rem Add Matsutake-3
adddrv @{devfile}

rem Change current drive
@{exedrv}
rem Change current directory
cd @{exedir}

rem Execute
@6{exefile}

rem Delete added character device
deldrv

[bat_kiri4]
echo off
rem set path=a:\kiriv4;%path%;

rem Add Matsutake-3
adddrv @{devfile}

rem Change current drive
@{exedrv}
rem Change current directory
cd @{exedir}

rem Execute
@6{exefile}

rem Delete added character device
deldrv

[bat_kiri4e]
echo off
rem set path=a:\kiriv4;%path%;

rem Add Matsutake-3
adddrv @{devfile}

rem Change current drive
@{exedrv}
rem Change current directory
cd @{exedir}

rem Execute
@6{exefile}

rem Delete added character device
deldrv

;**************************************** [dev_<devname>]セクション
[dev_vjeb25]
device = @{vjeb.drv} /t1 /m1 /j /l /hb /ks /kr /kg /k, /k. /k- /@3{vjeb.dic} /sys=@1{vjeb.drv}

[dev_yayoi_3]
device = @{vjeb.drv} /M5 /HR /L /KG /D2 /sys=@1{vjeb.drv}

[dev_pca_bps]
device = @{print.sys}
device = @{vjeb.drv} /m2 /hr /j /l /t0

[dev_vjeb30]
device = @{vjeb.drv} /L /K, /K. /K/ /K- /J /sys=@1{vjeb.drv}

[dev_vjepen3]
device = @{vjeb.drv} /j /k, /k. /k/ /k- /k[ /kx /l /d2 /sys=@1{vjeb.drv}

[dev_works25]
device = @{vjeb.drv} /HR /L /M1 /K, /K. /K- /K[ /EX /sys=@1{vjeb.drv}

[dev_kid30]
device = @{vje.sys} /N /T30
device = @{rsdrv.sys}

[dev_a_leter]
device = @{egb98.sys} /A/2/J/A/S/E/Y/1
device = @{egb98if.sys}

[dev_top2]
device = @{vjeb.drv} /@3{vjeb.dic} /i /j /m1 /HR /N /t0 /ks /kg /kr

[dev_katana4]
device = @{ktn4.sys} /E/AS0/AE128/AX0/AGN
device = @{ktn4c.sys} /E/H/D@{ktn.dic},@{usr.dic}/I111221/M3111/J11/C5CEDM/Z22222221/O11

[dev_atok7]
device=@{atok7a.SYS} /D=@{atok7.dic} /G=@{jfgaij.ufo}
device=@{atok7b.SYS}

[dev_atok7l]
device=@{atok7a.SYS} /D=@{atok7l.dic} /G=@{jfgaij.ufo}
device=@{atok7b.SYS}

[dev_jdash]
device=@{atok7a.SYS} /D=@{atok7d.dic} /G=@{jfgaij.ufo} /U=1
device=@{atok7b.SYS}

[dev_wperfect]
device = @{wpkb.sys}
device = @{wpfep.sys}

[dev_f1dbox]
device = @{jj2.sys} /p@1{jj2.sys}
device = @{rsdrv.sys}

[dev_matutake]
device = @{mttk2.drv}

[dev_mttk3]
device = @{mttk3a.drv} @1{mttk3a.drv} /J2
device = @{mttk3b.drv}
device = @{mcode.drv}

[dev_kiri4]
device = @{mttk3.drv} @1{mttk3.drv} /J2

[dev_diva]
device=@{vjeb.drv} /l /j /t1 /m1 /hb /k, /k. /k-

[dev_dynacad]
device=@{mouse.sys}
device=@{rsdrv.sys}
device=@{vjeb.drv} /@3{vjeb.dic} /l /t0 /m0 /hr /sys=@3{vjeb.drv}

[dev_dataease]
device=@{vjeb.drv} /l /j /t1 /m1 /hb /k, /k. /k-

[dev_pagepro3]
device=@{mouse.sys}

