; プリンタのデータ セクションの説明です。
;
; UpdateName              == .INIタイプ プロファイル,
;                            .INI設定セクション,
;                            デフォルト,
;                            .INIセクション フラグ,
;                            複数設定フラグ
;
; 各項目の説明:
;
; UpdateName              == このファイル内のプリンタ記述セクションの名前です。
;                            WIN.INIでは、[devices] がセクション名、UpdateNameが
;                            キー名になります。セットアップは、WIN.INIから
;                            "printer=4"キー名を変換するためにこの名前を参照
;                            します。
;
; .INIタイプ プロファイル == Win 3.0のWIN.INIのプリンタ設定情報セクション
;                            からセットアップがプリンタ記述インデックスを
;                            見つけるときに使う、プロファイル文字列です。
;                            (“.INI設定セクション”がセクション名のとき、
;                             この文字列はWIN.INIのキー名になります)。
;
; .INI設定セクション      == 各プリンタに対応する、Win 3.0のWIN.INIのプリンタ
;                            設定セクションです(ポート設定情報を除く)。
;
; デフォルト              == Win 3.0のWIN.INIからプリンタ記述プロファイルを
;                            取得できないときに、このファイルから記述文字列
;                            を取得ときに使うデフォルトのプロファイルです。
;                            これは、“設定されていないプリンタの場合”の
;                            ときに使われます。
;
; .INIセクション フラグ   == このフラグは、セットアップがポートの設定情報を
;                            使ってWin 3.0のWIN.INIのプリンタ設定セクション名
;                            を作成するかどうかを決めるものです。たとえば、
;                            HPPCLのセクション名であれば [HPPCL,port] のよう
;                            になり、EPSONの設定セクションであればつねにポート
;                            情報を持たない [epson9drv] のようになります。
;                            WIN.INIの設定セクションがポート情報を使わずに
;                            作成されるときには、このフラグを1にセットして
;                            ください。ポート情報を使うときはNULLのままに
;                            しておいてください。 
;
; 複数設定フラグ          == ドライバに対して単一のプリンタだけを設定するとき
;                            は、このフラグを1にセットしてください。ドライバが
;                            複数の設定セクションをセットアップできるときには、
;                            NULLのままにしておいてください。
;
; 単一モデルのドライバでは、指定されたモデル名文字列を
; セットアップが使うようにするため、用紙方向が使われます。
[Printer.Data]
"Canon BJ-10v/300J/330J"    = "model",        "Canon BJ-10v/300J/330J", "BJ-10v",1,1
"Canon LBP-B406S/D"         = "printer",      "Canon LBP-B406S/D,",     1
"EPSON (ESC/P)"             = "Printer Name", "EPSON (ESC/P)",          "AP300",1,1
"EPSON (ESC/Page)"          = "Model",        "EPSON (ESC/Page)",       7,1,1
"EPSON LP-7000/3000"        = "Model",        "EPSON LP-7000",          7,1,1
"EPSON (ESC/Page ﾋﾞｯﾄｲﾒｰｼﾞ)"= "Model",        "EPSON (ESC/Page ﾋﾞｯﾄｲﾒｰｼﾞ)",7,1,1
"HP DeskJet J-Series v1.0"  = "prtindex",     "DJ505J,",                0
"NEC NM"                    = "Model",        "NEC NM",                 NM2010,1,1
"NEC NPDL"                  = "Model",        "NEC NPDL",               PR2000,1,1
"NPDL Level2 Printer"       = "device",       "NPDL2,",                 2
"NEC PC-PR101/T PRINTER"    = "Prn",          "NEC PC-PR101/T PRINTER", 135,1,1
"NEC PC-PR150V PRINTER"     = "Prn",          "NEC PC-PR150V PRINTER",  138,1,1
"NEC PC-PR201"              = "Printer Model","NEC PC-PR201",           PR201H,1,1
"NEC PC-PR602"              = "Model",        "NEC PC-PR602",           PR602R,1,1
"EPSON PostScript"          = "device",       "PostScript,",            "EPSON LP-3000PS F2"
"OKI PostScript 78"         = "device",       "PostScript,",            1
"OKI PostScript 83"         = "device",       "PostScript,",            1
"RICOH PC LASER"            = "Model",        "RICOH PC LASER",         "SP4mk2",1,1

[Canon BJ-10v/300J/330J]
BJ-10v        = "Canon Bubble-Jet BJ-10v"
BJ-10v/Custom = "Canon Bubble-Jet BJ-10v Custom"
BJ-10v Select = "Canon Bubble-Jet BJ-10v Select"
BJ-15v        = "Canon Bubble-Jet BJ-15v"
BJ-300J       = "Canon Bubble-Jet BJ-300J"
BJ-330J       = "Canon Bubble-Jet BJ-330J"

[Canon LBP-B406S/D]
1 = "Canon LBP-B406S LIPS3"
2 = "Canon LBP-B406D LIPS3"
3 = "Canon LBP-A404 LIPS3"
4 = "Canon LBP-B406E LIPS3"
5 = "Canon LBP-A404E LIPS3"
6 = "Canon LBP-A304E LIPS3"
7 = "Canon LBP-B406G LIPS3"

[EPSON (ESC/P)]
AP1000  = "EPSON AP-1000"
AP300   = "EPSON AP-300"
AP500   = "EPSON AP-500"
AP800   = "EPSON AP-800"
AP900   = "EPSON AP-900"
FBP3000 = "EPSON FBP-3000"
HG2000  = "EPSON HG-2000"
HG4000  = "EPSON HG-4000"
HG5130  = "EPSON HG-5130"
HG800   = "EPSON HG-800"
VP1000  = "EPSON VP-1000"
VP1500  = "EPSON VP-1500"
VP2000  = "EPSON VP-2000"
VP2600  = "EPSON VP-2600"
VP300   = "EPSON VP-300"
VP4800  = "EPSON VP-4800"
VP800   = "EPSON VP-800"
VP900   = "EPSON VP-900"
XP2000  = "EPSON XP-2000"

[EPSON (ESC/Page)]
2 = "EPSON LP-2000"
3 = "EPSON LP-3000"
7 = "EPSON LP-7000/7000G"
8 = "EPSON LP-8000"

[EPSON LP-7000/3000]
2 = "EPSON LP-2000"
3 = "EPSON LP-3000"
7 = "EPSON LP-7000/7000G"
8 = "EPSON LP-8000"

[EPSON (ESC/Page ﾋﾞｯﾄｲﾒｰｼﾞ)]
2 = "EPSON LP-2000"
3 = "EPSON LP-3000"
7 = "EPSON LP-7000/7000G"
8 = "EPSON LP-8000"

[HP DeskJet J-Series v1.0]
; Windows 3.1 HP DeskJet 505J driver not support Color
; 0 = "HP DeskJet 505J"
1 = "HP DeskJet 500J"

[EPSON PostScript]
"EPSON LP-3000PS F2" = "EPSON LP-3000PS F2"
"EPSON LP-3000PS F5" = "EPSON LP-3000PS F5"

[OKI PostScript 78]
1 = "OKI MICROLINE 801PS"
2 = "OKI MICROLINE 801PS+F"
3 = "OKI OPP6008PS"
"OKI ML801PS"                = "OKI MICROLINE 801PS"
"OKI ML801PS (漢字)"         = "OKI MICROLINE 801PS"
"OKI ML801PS (漢字２書体)"   = "OKI MICROLINE 801PS"
"OKI ML801PS+F"              = "OKI MICROLINE 801PS+F"
"OKI ML801PS+F (漢字)"       = "OKI MICROLINE 801PS+F"
"OKI ML801PS+F (漢字５書体)" = "OKI MICROLINE 801PS+F"
"OKI OPP6008PS"              = "OKI OPP6008PS"
"OKI OPP6008PS (漢字)"       = "OKI OPP6008PS"
"OKI OPP6008PS (漢字２書体)" = "OKI OPP6008PS"

[OKI PostScript 83]
1 = "OKI MICROLINE 801PS"
2 = "OKI MICROLINE 801PS+F"
3 = "OKI OPP6008PS"
"OKI ML801PS"                = "OKI MICROLINE 801PS"
"OKI ML801PS (漢字)"         = "OKI MICROLINE 801PS"
"OKI ML801PS (漢字２書体)"   = "OKI MICROLINE 801PS"
"OKI ML801PS+F"              = "OKI MICROLINE 801PS+F"
"OKI ML801PS+F (漢字)"       = "OKI MICROLINE 801PS+F"
"OKI ML801PS+F (漢字５書体)" = "OKI MICROLINE 801PS+F"
"OKI OPP6008PS"              = "OKI OPP6008PS"
"OKI OPP6008PS (漢字)"       = "OKI OPP6008PS"
"OKI OPP6008PS (漢字２書体)" = "OKI OPP6008PS"

[NEC NM]
NM2010 = "NEC NM-2010"
NM4150 = "NEC NM-4150"
NM9950 = "NEC NM-9950/9950II"
NM5020 = "NEC NM-5020/5020L"
NM9700 = "NEC NM-9700"
NM9900 = "NEC NM-9900"

[NEC NPDL]
PR601  = "NEC PC-PR601"
PR602  = "NEC PC-PR602"
PR602R = "NEC PC-PR602R"
PR1000 = "NEC PC-PR1000"
PR2000 = "NEC PC-PR2000"

[NPDL Level2 Printer]
1 = "NEC PC-PR1000/4"
2 = "NEC PC-PR2000/2"
3 = "NEC PC-PR2000/4"
4 = "NEC PC-PR4000/4"
5 = "NEC PC-PR4000E/4"

[NEC PC-PR101/T PRINTER]
135 = "NEC PC-PR201/TC100"
138 = "NEC PC-PR101/T67"

[NEC PC-PR150V PRINTER]
135 = "NEC PC-PR350"
137 = "NEC PC-PR150VH"
138 = "NEC PC-PR150V"
139 = "NEC PC-PR150T"
146 = "NEC PC-PR150N"

[NEC PC-PR201]
PR201L = "NEC PC-PR201"
PR201M = "NEC PC-PR201"
PR201H = "NEC PC-PR201"
PR101L = "NEC PC-PR101"
PR101  = "NEC PC-PR101"

[NEC PC-PR602]
PR601  = "NEC PC-PR601"
PR602  = "NEC PC-PR602"
PR602R = "NEC PC-PR602R"
PR1000 = "NEC PC-PR1000"
PR2000 = "NEC PC-PR2000"

[RICOH PC LASER]
SP4    = "RICOH PC-LASER SP4mkII"
SP4mk2 = "RICOH PC-LASER SP4mkII"
SP5    = "RICOH PC-LASER SP5"

;
; このセクションは、.WPDファイルから抜きとられたプリンタの記述文字列を
; "プリンタの正式名称"に容易に変換するためのものです。WPDプリンタの名前は
; CONTROL.INFにリストされているプリンタ名と一致しないことがあるため、この
; セクションを使ってプリンタ名を適切に更新します。
;
; "WPD記述プレフィックス",    "プリンタの正式名称"
;
; コードは、以下に見られる第1フィールドの1〜N番目の文字に対して、WPD記述
; 文字列と一致しているかどうかをチェックします。一致する文字列が見つかると、
; コードは第2フィールドの記述文字列とそのプリンタ名を利用します。
;
[WPD_NickNames]
"Apple LaserWriter II NTX-J",  "Apple LaserWriter II NTX-J"
"Canon LBP-A404PS Lite",       "Canon LBP-A404PS Lite"
"Canon LBP-A404PS",            "Canon LBP-A404PS"
"EPSON LP-3000PS F2",          "EPSON LP-3000PS F2"
"EPSON LP-3000PS F5",          "EPSON LP-3000PS F5"
"Fujitsu FMLBP211PS",          "Fujitsu FMLBP211PS"
"NEC PC-PR3000PS/4F 400dpi",   "NEC PC-PR3000PS/4F 400dpi"
"NEC PC-PR3000PS/4 400dpi",    "NEC PC-PR3000PS/4 400dpi"
"NEC PC-PR3000PS 320dpi",      "NEC PC-PR3000PS 320dpi"
"NEC PC-PR602PS 320dpi",       "NEC PC-PR602PS 320dpi"
"NEC PC-PR800PS/3",            "NEC PC-PR800PS/3"
"OKI MICROLINE 801PS+F",       "OKI MICROLINE 801PS+F"
"OKI MICROLINE 801PS",         "OKI MICROLINE 801PS"
"OKI OPP6008PS",               "OKI OPP6008PS"
