;***************************************************************************/
;*                                                                         */
;* OEMSETUP.INF                                                            */
;*                                                                         */
;*                  Copyright (c) Madge Networks Ltd. 1994                 */
;*                                                                         */
;* Date: Wed 09th Feb 1994                                                 */
;* Author: aclc                                                            */
;*                                                                         */
;* MADGE Smart Ringnode Driver installer                                   */
;*                                                                         */
;***************************************************************************/
;
; v1.08
;
; For use with SmartNT.sys v1.14
; 
;-----------------------------------------------------------------------

[Identification]
    OptionType = NetAdapter

;-----------------------------------------------------------------------
; PlatformsSupported
; ------------------
; This identifies the platforms supported by the adapter card.
; Possible types are:
;
; ISA, EISA and MCA
;-----------------------------------------------------------------------

[PlatformsSupported]
    MCA
    ISA
    EISA
    "Jazz-Internal Bus"

;-----------------------------------------------------------------------
; LANGUAGES SUPPORTED
; -------------------
;
; The languages supported by the OEM INF, For every language supported
; we need to have a separate text section for every displayable text
; section.
;
;-----------------------------------------------------------------------

[LanguagesSupported]
    ENG

;-----------------------------------------------------------------------
; OPTION LIST
; -----------
; This section lists the OEM Option key names.  These keys are locale
; independent and used to represent the option in a locale independent
; manner.
;
;-----------------------------------------------------------------------

[Options]
    MDGMCA
    MDGEISA
    MDGISA

;-----------------------------------------------------------------------
; OPTION TEXT SECTION
; -------------------
; These are text strings used to identify the option to the user.  There
; are separate sections for each language supported.  The format of the
; section name is "OptionsText" concatenated with the Language represented
; by the section.
;
;-----------------------------------------------------------------------

[OptionsTextENG]
    MDGMCA      = "Madge Smart 16/4 Ringnode (MCA)"
    MDGEISA     = "Madge Smart 16/4 Ringnode (EISA)"
    MDGISA      = "Madge Smart 16/4 Ringnode (ISA)"


;***********************************************************************
; CONSTANTS FOR USING DIALOGS
;***********************************************************************

[IRQChoices]
IRQ_1 = "02",2
IRQ_2 = "03",3
IRQ_3 = "05",5
IRQ_4 = "07",7
IRQ_5 = "10",10
IRQ_6 = "11",11
IRQ_7 = "12",12
IRQ_8 = "15",15


[IOLocationChoices]
IOBase_1  = "0x0a20",2592
IOBase_2  = "0x1a20",6688
IOBase_3  = "0x2a20",10784
IOBase_4  = "0x3a20",14880
IOBase_5  = "0x4a20",18976
IOBase_6  = "0x4e20",20000
IOBase_7  = "0x6a20",27168
IOBase_8  = "0x6e20",28192


[DMAChannelChoices]
DMAChannel_1  = "PIO",0
DMAChannel_2  = "01",1
DMAChannel_3  = "03",3
DMAChannel_4  = "05",5
DMAChannel_5  = "06",6


[FileConstants]
;
;  File names, etc.
;
UtilityInf        = "UTILITY.INF"
subroutineinf     = "SUBROUTN.INF"
SoftwareType      = "driver"
Exit_Code         = 0
DialogDllName     = "madgedlg.dll"

; Product Info
;
Manufacturer        = "Madge"
ProductMajorVersion = "1"
ProductMinorVersion = "10"
ProductVersion      = $(ProductMajorVersion)"."$(ProductMinorVersion)
;
; Software
;
ProductSoftwareName     = "SMARTNT"
ProductSoftwareImagePath = "%SystemRoot%\system32\drivers\"$(ProductSoftwareName)".sys"

NetRuleSoftwareType     = "mdgtrSys ndisDriver mdgtrDriver"
NetRuleSoftwareUse      = $(SoftwareType)
NetRuleSoftwareBindForm = """mdgtrSys"" yes no container"
NetRuleSoftwareClass    = {"mdgtrDriver basic"}
NetRuleSoftwareBindable = {"mdgtrDriver mdgtrAdapter non exclusive 100"}
;
; Hardware
;
ProductHardwareName         = "SMARTNT"
NetRuleHardwareType         = "mdgtr mdgtrAdapter"
NetRuleHardwareBindForm     = " yes yes container"
NetRuleHardwareClass        = {"mdgtrAdapter basic"}
;
; Registry Key
;
ProductKeyName  = $(!NTN_SoftwareBase)"\"$(Manufacturer)"\"$(ProductSoftwareName)"\CurrentVersion"
ParamKeyName    = $(!NTN_ServiceBase)"\"$(ProductHardwareName)"\Parameters"
;
; EventLog Message File
;
; (This is a bit naughty - we ought really to have a separate Event Log file,
;  but this is just a first pass, so we will leave it as is for now.)
;
MadgeEventLogFile = $(ProductSoftwareImagePath)


[GeneralConstants]
;
;  Program flow control variables.
;
from      = ""
to        = ""
;
;  Return codes; Exit_Code is set to one of these
;
ExitCodeOk     = 0
ExitCodeCancel = 1
ExitCodeFatal  = 2

MAXIMUM_ALLOWED    = 33554432
RegistryErrorIndex = NO_ERROR
KeyNull            = ""
KeyProduct         = ""
KeyParameters      = ""

TRUE            = 1
FALSE           = 0
NoTitle         = 0

ExitState         = "Active"
OldVersionExisted = $(FALSE)

DriverPath      = $(!STF_NTPATH)\drivers

IRQList  = ^(IRQChoices, 1)
IRQValues = ^(IRQChoices, 2)

IOLocationList = ^(IOLocationChoices, 1)
IOLocationValues = ^(IOLocationChoices, 2)

DMAChannelList = ^(DMAChannelChoices,1)
DMAChannelValues = ^(DMAChannelChoices,2)

MadgeHelpIdMin     = 6000
MadgeHelpIdMax     = 6002
MadgeHelpIdMDGISA  = 6001
MadgeHelpIdMDGEISA = 6002
MadgeHelpIdMDGMCA  = 6002


;***********************************************************************
; Language-Dependent Dialog Constants
;***********************************************************************

[FileConstantsENG]
;
;  Variables to support thermometer gauge and error dialogs
;
;ProCaption   = "Windows NT Setup"
;ProCancel    = "Cance&l"
;ProCancelMsg = "Windows NT Networking is not correctly installed.  "+
;               "Are you sure you want to cancel copying files?"

;ProCancelCap = "Network Setup Message"
;ProText1     = "Copying:"
;ProText2     = "To:"

;
; Product Info
;
FunctionTitle   = "Madge Smart 16/4 Ringnode Setup"
;
; Software
;
ProductSoftwareTitle       = "Madge Smart 16/4 Ringnode Driver"
ProductSoftwareDescription = "Madge Smart 16/4 Ringnode NDIS3 Driver"
;
; Hardware
;
ProductHardwareMDGMCATitle  = "Madge Smart 16/4 MCA Ringnode"
ProductHardwareMDGEISATitle = "Madge Smart 16/4 EISA Ringnode"
ProductHardwareMDGISATitle  = "Madge Smart 16/4 ISA Ringnode"
ProductHardwareMDGMCADescription  = "Madge Smart 16/4 Ringnode (MicroChannel)"
ProductHardwareMDGEISADescription = "Madge Smart 16/4 Ringnode (EISA Bus)"
ProductHardwareMDGISADescription  = "Madge Smart 16/4 Ringnode (ISA Bus)"

CANNOT_FIND_ANY_CARD = "Network card is not present in the system"
TRIMMED_MFS = "WARNING: The maximum frame size at 16Mbps is 17839 bytes"+
	      "  and you have specified a value greater than that. This"+
	      "  value has been reduced to 17839 for you. If you are in"+
	      "  fact running at 4Mbps, the maximum frame size is 4472,"+
	      "  but do not worry -  the driver will automatically  set"+
	      "  the correct value, and write it to the Event Log."

ShellCodeErrorTitle = "Error: "$(FunctionTitle)
ShellCodeErrorText  = "Shell Code Error"

[DialogConstantsENG]
;
; Common button names, etc.
;
Help        = "&Help"
Exit        = "&Cancel"
OK          = "&OK"
Continue    = "C&ontinue"
Cancel      = "C&ancel"
HelpContext = ""

[date]
    ; Now is a list which contains { Sec from 1-1-1970, Year, Month, Day, Hour,
    ; Minute, Second }
    Now = {} ? $(!LIBHANDLE) GetSystemDate


;-----------------------------------------------
; Input DIALOGS
;-----------------------------------------------

[FileDependentDlgENG]
DlgType     = "RadioCombination"
DlgTemplate = $(Option)

Caption = $(FunctionTitle)

;DlgText = "Please select values for the following fields:"

Combo1Label = "&IRQ Level:"
Combo2Label = "I/O &Loc/Slot:"
Combo3Label = "DMA &Channel:"

Combo1List = $(IRQList)
Combo1Out  = $(IRQValue)

Combo2List = $(IOLocationList)
Combo2Out  = $(IOLocationValue)

Combo3List = $(DMAChannelList)
Combo3Out  = $(DMAChannelValue)

ComboListItemsIn  = {Combo1List, Combo2List, Combo3List}
ComboListItemsOut = {Combo1Out, Combo2Out, Combo3Out}

Edit1Label  = "MaxFrameSize:"
Edit2Label  = "LAA:"
EditTextIn  = {$(MaxFrameSize), $(LAA)}
EditTextLim = {5,17}
EditTextOut = {}

CBOptionsGreyed = {}
NotifyFields = {NO, NO, NO}

HelpContext = $(MadgeHelpId$(Option))


[MDGMCA_Bytes]
; Format of list items : { LoByte, HiByte }

; First generation 4Mbps only  {  3, 8}
; Second generation 4Mbps only { 14, 8}
; 16/4 standard model  (MC16)  { 45, 0}
; 16/4 streaming model (MC32)  {116, 0}

MDGMCA_ByteList = {+
		    {  3, 8 },+
		    { 14, 8 },+
		    { 45, 0 },+
		    {116, 0 } +
		  }

[MDGEISA_Bytes]
; EISAFindBus only appears to work if you specify the low three bytes of the
; compressed Id. The mask parameter appears to be unused. This makes our life
; much easier, because all EISA card Id's are the same in these bytes!

MDGEISA_LowWord = 34612 ; 0x00008734 MDG bit only

;---------------------------------------------------------------------------
; 1. Identify
;
; DESCRIPTION:   To verify that this INF deals with the same type of options
;                as we are choosing currently.
;
; INPUT:         None
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL
;                $($R1): Option Type (COMPUTER ...)
;                $($R2): Diskette description
;---------------------------------------------------------------------------

[Identify]
    ;
    ;
    read-syms Identification

    set Status     = STATUS_SUCCESSFUL
    set Identifier = $(OptionType)
    set Media      = #("Source Media Descriptions", 1, 1)

    Return $(Status) $(Identifier) $(Media)

;------------------------------------------------------------------------
; 2. ReturnOptions:
;
; DESCRIPTION:   To return the option list supported by this INF and the
;                localised text list representing the options.
;
;
; INPUT:         $($0):  Language used. ( ENG | FRN | ... )
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL |
;                                STATUS_NOLANGUAGE
;                                STATUS_FAILED
;                                STATUS_NOTSUPPORTED
;
;                $($R1): Option List
;                $($R2): Option Text List
;------------------------------------------------------------------------

[ReturnOptions]
    ;
    ;
    set Status         = STATUS_FAILED
    set OptionList     = {}
    set OptionTextList = {}

    ;
    ; Check if the language requested is supported
    ;
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) in $(LanguageList)
	;
	; Check if the platforms requested is supported
	;
	ifstr(i) $($1) == ""
			goto returnoptions
	endif

	set PlatformList = ^(PlatformsSupported, 1)
	Ifcontains(i) $($1) in $(PlatformList)
			goto returnoptions
	else
			set Status = STATUS_NOTSUPPORTED
			goto finish_ReturnOptions
	endif
    else
		set Status = STATUS_NOLANGUAGE
		goto finish_ReturnOptions
    endif

    ;
    ; form a list of all the options and another of the text representing
    ;

returnoptions = +
    set OptionList     = ^(Options, 1)
    set OptionTextList = ^(OptionsText$($0), 1)
    set Status         = STATUS_SUCCESSFUL

finish_ReturnOptions = +
    Return $(Status) $(OptionList) $(OptionTextList)

;------------------------------------------------------------------------
;
; InstallOption:
;
;      This section is shelled to by main installation processing
;      or by NCPASHEL.INF during reconfig, removal, update, etc.
;
;
; FUNCTION:  To copy files representing Options
;            To configure the installed option
;            To update the registry for the installed option
;
; INPUT:     $($0):  Language to use
;            $($1):  OptionID to install
;            $($2):  SourceDirectory
;            $($3):  AddCopy  (YES | NO)
;            $($4):  DoCopy   (YES | NO)
;            $($5):  DoConfig (YES | NO)
;
; OUTPUT:    $($R0): STATUS: STATUS_SUCCESSFUL |
;                            STATUS_NOLANGUAGE |
;                            STATUS_USERCANCEL |
;                            STATUS_FAILED
;
;------------------------------------------------------------------------
[InstallOption]

    StartWait
    ;
    ; Set default values for
    ;
    set Status   = STATUS_FAILED
    ;
    ; extract parameters
    ;
    set Option   = $($1)
    set SrcDir   = $($2)
    set AddCopy  = $($3)
    set DoCopy   = $($4)
    set DoConfig = $($5)

    Debug-Output "OEMSETUP.INF: STF_CWDIR is: "$(!STF_CWDIR)
    Debug-Output "OEMSETUP.INF: STF_LANGUAGE is: "$(!STF_LANGUAGE)

    ;
    ; Check if the language requested is supported
    ;
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) NOT-IN $(LanguageList)
	Return STATUS_NOLANGUAGE
    endif

    ; define all the constants

    set-subst LF = "\n"

    read-syms GeneralConstants
    read-syms FileConstants
    read-syms DialogConstants$(!STF_LANGUAGE)
    ifstr(i) $(!NTN_Origination) == "NCPA"
	set Continue = $(OK)
    endif
    read-syms FileConstants$(!STF_LANGUAGE)

    ifstr(i) $(Option) == "MDGMCA"
	set McaEisaKeyword = "McaPosId"
    else-ifstr(i) $(Option) == "MDGEISA"
	set McaEisaKeyword = "EisaCompressedId"
    endif

    SetHelpFile "madgedlg.hlp" $(MadgeHelpIdMin) $(MadgeHelpIdMax)

    detect date

    set-title  $(FunctionTitle)

    set to   = Begin
    set from = Begin
;
;  Assume all is well.
;
    set CommonStatus = STATUS_SUCCESSFUL

    EndWait

;
;   Set up the operation-mode-based variables and gaily welcome
;   the user.  If the "install mode" variable is improperly set,
;   assume this is a new installation.
;

Begin = +
    Debug-Output "SMARTNT: Install mode = "$(!NTN_InstallMode)
    Debug-Output "SMARTNT: Registry base = "$(!NTN_RegBase)

    Ifstr(i) $(!NTN_InstallMode) == deinstall
		set StartLabel = removeadapter
    else-Ifstr(i) $(!NTN_InstallMode) == Update
	set StartLabel = UpgradeSoftware
    else-Ifstr(i) $(!NTN_InstallMode) == bind
		set StartLabel = bindingadapter
    else-Ifstr(i) $(!NTN_InstallMode) == configure
		set CommonStatus = STATUS_REBOOT
		set StartLabel = configureadapter
		;
		;   You cannot config the software component
		;
		Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
			Debug-Output "Cannot configure the SmartNT driver software."
			Shell $(UtilityInf),RegistryErrorString,CANNOT_CONFIGURE_SOFTWARE
			ifint $($ShellCode) != $(!SHELL_CODE_OK)
				Debug-Output "ShellCode error: cannot get an error string."
				goto ShellCodeError
			endif
			set Error = $($R0)
			set from = end
			set to = end
			goto nonfatalinfo
		endif
    else
		set StartLabel = installadapter
		set OEM_ABANDON_OPTIONS = {}
		set OEM_ABANDON_SOFTWARE = FALSE
		set OEM_ABANDON_ON = TRUE
    endif

    set from = fatal
    set to   = fatal
    goto $(StartLabel)

;-----------------------------------------------
; Installation Section
;-----------------------------------------------

installadapter = +
;
;   First, check whether the same version of the software exists
;

    OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct

    Ifstr $(KeyProduct) != $(KeyNull)
	;
	; Same version already existed in the local machine
	; Popup the dialog and ask the user whether he wants to continue
	;
	CloseRegKey $(KeyProduct)

	ifstr(i) $(!NTN_RegBase) == $(ProductKeyName)
	   ;
	   ; Cannot Install the same software again
	   ;
	   Shell $(UtilityInf), VerExistedDlg, $(ProductSoftwareTitle),+
	       $(ProductVersion)
	   ifint $($ShellCode) != $(!SHELL_CODE_OK)
	       Debug-Output "ShellCode error: cannot get an error string."
	       goto ShellCodeError
	   endif

	   goto end
	else
	   ;
	   ; Add a new adapter card?
	   ;
	   Shell $(UtilityInf), CardExistedDlg

	   ifint $($ShellCode) != $(!SHELL_CODE_OK)
	       Debug-Output "ShellCode error: cannot get an error string."
	       goto ShellCodeError
	   endif

	   ifstr(i) $($R1) != "OK"
	       goto end
	   endif

	   set OldVersionExisted = $(TRUE)
	endif
    endif

    ifstr(i) $(Option) == "MDGMCA"
	set cardlist = {}
	read-syms MDGMCA_Bytes

	ForListDo $(MDGMCA_ByteList)
	    set MDGMCA_Elt_LoByte = *($($), 1)
	    set MDGMCA_Elt_HiByte = *($($), 2)

	    Shell $(UtilityInf) MCAFindBus $(MDGMCA_Elt_LoByte) $(MDGMCA_Elt_HiByte)
	    ifint $($ShellCode) != $(!SHELL_CODE_OK)
		goto ShellCodeError
	    endif
	    ifstr $($R0) != "NO_ERROR"
		set Error = $($R0)
		goto fatal
	    endif
	    ifstr(i) $($R1) != {}
		ifstr(i) $(cardlist) == {}
		    set cardlist = $($R1)
		else
		    set cardlist = >($(cardlist), $($R1))
		endif
	    endif

	EndForListDo

	ifstr(i) $(cardlist) == {}
	    set Error = $(CANNOT_FIND_ANY_CARD)
	    set CommonStatus = STATUS_USERCANCEL
	    set from = end
	    goto nonfatal
	endif
	set AdapterList = $(cardlist)
    else-ifstr(i) $(Option) == "MDGEISA"
	set cardlist = {}
	read-syms MDGEISA_Bytes

	Shell $(UtilityInf) EISAFindBus $(MDGEISA_LowWord)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    goto ShellCodeError
	endif
	ifstr $($R0) != "NO_ERROR"
	    set Error = $($R0)
	    goto fatal
	endif
	ifstr(i) $($R1) != {}
	    set cardlist = $($R1)
	endif

	ifstr(i) $(cardlist) == {}
	    set Error = $(CANNOT_FIND_ANY_CARD)
	    set CommonStatus = STATUS_USERCANCEL
	    set from = end
	    goto nonfatal
	endif
	set AdapterList = $(cardlist)
    else
	; Must be an ISA card - nothing to look for here.
	; Instead, we have to ask the user for the IO Location/Irq number/Dma
	; channel. This happens down below.

    endif

    ifstr(i) $(Option) != "MDGISA"
	; For MCA/EISA cards, determine the slot number and id of the card

	ForListDo $(AdapterList)
	    set BusNum      = *($($), 1)
	    set SlotNum     = *($($), 2)
	    set Mca_Eisa_Id = *($($), 3)
	    Shell $(UtilityInf) IsNetCardAlreadyInstalled $(BusNum) $(SlotNum) +
		$(ProductHardware$(Option)Description) $(ProductHardwareName)
	    ifint $($ShellCode) != $(!SHELL_CODE_OK)
		goto ShellCodeError
	    endif
	    ifstr $($R0) != "NO_ERROR"
		set Error = $($R0)
		goto fatal
	    endif
	    ifstr(i) $($R1) != "YES"
		set SlotNumber = $(SlotNum)
		set McaEisaId  = $(Mca_Eisa_Id)
		goto installdll
	    endif
	EndForListDo

	; If we get here, we have failed to find the new card, so we had better
	; fail.

	set Error        = $(CANNOT_FIND_ANY_CARD)
	set CommonStatus = STATUS_USERCANCEL
	set from         = end
	goto nonfatal

    endif ; $(Option) != MDGISA

;
;  dll load addition
;     If the software is not already installed, we must install the .DLL file
;  so that we can query the user for ISA parameters and MFS/LAA values
;
installdll = +

    ifint $(OldVersionExisted) == $(FALSE)
	ifstr(i) $(!NTN_InstallMode) == "install"
	    ifstr(i) $(DoCopy) == "YES"

; NB !STF_SRCDIR is set to something unhelpful like E:\i386\, but if we
;    omit the last parameter, DoAskSource will default to using A:\
;
;       Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(!STF_SRCDIR)

		Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR)

		Ifint $($ShellCode) != $(!SHELL_CODE_OK)
		    Goto ShellCodeError
		Else-Ifstr(i) $($R0) == STATUS_FAILED
		    shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
		    ifint $($ShellCode) != $(!SHELL_CODE_OK)
			goto ShellCodeError
		    endif
		    set Error = $($R0)
		    Goto fatal
		Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
		    Goto successful
		Endif

		Set SrcDir = $($R1)   ; Referenced in [Install-Dll]

	    endif

	    install "Install-Dll"

	    ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
		shell $(UtilityInf) RegistryErrorString "UNABLE_COPY_FILE"
		ifint $($ShellCode) != $(!SHELL_CODE_OK)
		    goto ShellCodeError
		endif
		set Error = $($R0)
		goto fatal
	    endif
	endif
    endif

    ; Set some defaults that apply to all card types

    set MaxFrameSize = 2436

    set LAA = ""

    ;  set the default values that apply only to ISA cards

    set IRQValue = *($(IRQList), 6)

    set IOLocationValue = *($(IOLocationList), 1)

    set DmaChannelValue = *($(DMAChannelList), 3)

    goto adapteroptions


;-----------------------------------------------
; Configuration Section
;-----------------------------------------------
;
;   Get the current values of all the parameters
;
configureadapter = +
    ; NB !NTN_RegBase, for hardware components, is :
    ;    \SOFTWARE\Microsoft\Windows NT\CurrentVersion\NetworkCards\0x

    ; This next IF is redundant - it will always be NULL
    Ifstr $(KeyProduct) == $(KeyNull)
	OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) $(MAXIMUM_ALLOWED) KeyProduct
	Ifstr $(KeyProduct) == $(KeyNull)
	    set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
	    Debug-Output "Cannot find component product key"
	    goto fatalregistry
	Endif
    Endif

    ;
    ; Get the other parameters;  they're attached to the service parameters key
    ;

    Shell $(UtilityInf) FindService, $(KeyProduct)
    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
		Debug-Output "INF: FindService shell failure"
		Goto ShellCodeError
    Endif
    Ifstr(i) $($R0) != NO_ERROR
		Debug-Output "INF: FindService Shell error: "$($R0)
		Goto fatalregistry
    endif

    set KeyParameters = $($R2)

    ;
    ;  We don't need the services key, so close it.
    ;
    CloseRegKey $($R1)

    Ifstr $(KeyParameters) == $(KeyNull)
		set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
		Debug-Output "Cannot find component service"
		goto fatalregistry
    endif

    set OldVersionExisted = $(TRUE)

    set ValueName = ""
    set ValueData = ""
    set ValueStr  = ""
    set ValueList = {}

    ;
    ; Get the old values
    ;
    EnumRegValue $(KeyParameters) ValueList

    ForListDo $(ValueList)
	set ValueItem = $($)
	set ValueName = *($(ValueItem),1)
	set ValueData = *($(ValueItem),4)

	ifstr(i) $(ValueName) == "InterruptNumber"
	    set IRQValueIndex = $(ValueData)
	else-ifstr(i) $(ValueName) == "IoLocation"
	    set IOLocationIndex = $(ValueData)
	else-ifstr(i) $(ValueName) == "DmaChannel"
	    set DMAChannelIndex = $(ValueData)
	else-ifstr(i) $(ValueName) == "SlotNumber"
	    set SlotNumber = $(ValueData)
	else-ifstr(i) $(ValueName) == $(McaEisaKeyword)
	    set McaEisaId = $(ValueData)
	else-ifstr(i) $(ValueName) == "MaxFrameSize"
	    set MaxFrameSize = $(ValueData)
	else-ifstr(i) $(ValueName) == "NetworkAddress"
	    set LAA = $(ValueData)
	endif

    EndForListDo

    ifstr $(Option) == MDGISA
	; If it is NOT MDGISA, we don't care about any of these values.

	set IRQValue = *($(IRQList), ~($(IRQValues),$(IRQValueIndex)))
	ifstr(i) $(IRQValue) == ""
	    set IRQValue = *($(IRQList), 6)
	endif

	set DMAChannelValue = *($(DMAChannelList), ~($(DMAChannelValues),$(DMAChannelIndex)))
	ifstr(i) $(DMAChannelValue) == ""
	    set DMAChannelValue = *($(DMAChannelList), 4)
	endif

	set IOLocationValue = *($(IOLocationList), ~($(IOLocationValues),$(IOLocationIndex)))
	ifstr(i) $(IOLocationValue) == ""
	    set IOLocationValue = *($(IOLocationList), 1)
	endif

    endif ; $(Option) == MDGISA

;
;   Let the user bang on the options until satisfied.
;
adapteroptions = +
    set from = adapteroptions

    set oldLAA = $(LAA)

    ; This will set DlgTemplate to be the same as $(Option)

    read-syms FileDependentDlg$(!STF_LANGUAGE)

    ; MDGEISA and MDGMCA share the same dialog

    ifstr(i) $(Option) == "MDGMCA"
	set DlgTemplate = "MDGEISA"
    endif

    LoadLibrary "Disk 1" $(DialogDllName) MdgDialog

    ui start "InputDlg"  $(MdgDialog)

    ifstr(i) $(DLGEVENT) == "CONTINUE"
		ifstr $(Option) == MDGISA
		    set IRQValueIndex   = $(Combo1Out)
		    set IOLocationIndex = $(Combo2Out)
		    set DMAChannelIndex = $(Combo3Out)
		endif
		set MaxFrameSize    = *($(EditTextOut), 1)
		set LAA             = *($(EditTextOut), 2)
		ui pop 1
		goto adapterverify
    else-ifstr(i) $(DLGEVENT) == "EXIT"
		set CommonStatus = STATUS_USERCANCEL
		Debug-Output "Action: exit. Bye."
		ui pop 1
		FreeLibrary $(MdgDialog)
		goto end
    else
		;
		; Unknow command
		;
		ui pop 1
		Debug-Output "Action: unknown. Bye."
		FreeLibrary $(MdgDialog)
		goto end
    endif

adapterverify = +

    ifstr $(LAA) != ""

	; NB A line of spaces will come through here, and will fail the
	;    check - do we want this?

	Debug-Output "LAA non-null - will check it"

	set FLibraryErrCtl = 1

	LibraryProcedure MdgResult $(MdgDialog) MadgeLAACheck $(LAA)

	set FLibraryErrCtl = 0

	ifstr $(MdgResult) != "MADGE_STATUS_SUCCESS"
	    ; Illegal LAA supplied in the install dialog
	    ; Display error message and go around again
	    FreeLibrary $(MdgDialog)
	    set Error = $(MdgResult)
	    goto nonfatal ; this will go back to "adapteroptions", or to "end"
	endif

    endif

    FreeLibrary $(MdgDialog)

    ifint $(MaxFrameSize) > 17839
    ; 17839 is the maximum frame size at 16Mbps, while at 4Mbps it is 4472.
    ; Unfortunately, we can't tell here what the ring speed is, so guess at
    ; 16Mbps, which is the most sensible.
	set MaxFrameSize = 17839
	set Error = $(TRIMMED_MFS)
	set from = checkedMFS
	goto nonfatalinfo
    endif

checkedMFS = +
;
;   If installing, go create the necessary keys;
;   if configuring, they're already open.
;
    ifint $(OldVersionExisted) == $(TRUE)
	ifstr(i) $(!NTN_InstallMode) == configure
	    goto writeparameters
	endif
    endif

    StartWait

    ;
    ; Add Software Component
    ;
    ifint $(OldVersionExisted) == $(FALSE)
	ifstr(i) $(!NTN_InstallMode) == "install"
	    Ifstr(i) $(DoCopy) == "YES"

;            Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(!STF_SRCDIR)
		Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR)

		Ifint $($ShellCode) != $(!SHELL_CODE_OK)
		    Goto ShellCodeError
		Else-Ifstr(i) $($R0) == STATUS_FAILED
		    Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
		    ifint $($ShellCode) != $(!SHELL_CODE_OK)
			goto ShellCodeError
		    endif
		    set Error = $($R0)
		    Goto fatal
		Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
		    Goto successful
		Endif

		Set SrcDir = $($R1)   ; Referenced in Install-Option

	    endif

	    install "Install-Driver"

	    ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
		shell $(UtilityInf) RegistryErrorString "UNABLE_COPY_FILE"
		ifint $($ShellCode) != $(!SHELL_CODE_OK)
		    goto ShellCodeError
		endif
		set Error = $($R0)
		goto fatal
	    endif
	Endif

	Shell $(UtilityInf), AddSoftwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), +
	    $(ProductSoftwareName), +
	    $(ProductSoftwareTitle), $(STF_CONTEXTINFNAME), +
	    $(ProductSoftwareImagePath), "kernel", "NDIS", {}, "",+
	    $(MadgeEventLogFile)

	Set OEM_ABANDON_SOFTWARE = TRUE

	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif
	;
	;   At this point:
	;     $R1 contains the product version key handle;
	;     $R2 contains the NetRules subkey handle;
	;     $R3 contains the new Services key handle; and
	;     $R4 contains the Parameters key
	;     $R5 contains the Linkage Key
	;
	set RegistryErrorIndex = $($R0)
	set KeyProduct      = $($R1)
	Set SoftNetRulesKey = $($R2)
	CloseRegKey $($R3)
	CloseRegKey $($R4)
	CloseRegKey $($R5)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    EndWait
	    Debug-Output "Registry error: add software components"
	    CloseRegKey $(KeyProduct)
	    CloseRegKey $(SoftNetRulesKey)
	    goto fatalregistry
	endif

	set NewValueList = {{SoftwareType,$(NoTitle),$(!REG_VT_SZ),$(SoftwareType)},+
			   {MajorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMajorVersion)},+
			   {MinorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMinorVersion)},+
			   {Title,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareTitle)},+
			   {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareDescription)},+
			   {PathName,$(NoTitle),$(!REG_VT_SZ),$(!STF_CWDDIR)},+
			   {ServiceName,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareName)},+
			   {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}

	Shell  $(UtilityInf), AddValueList, $(KeyProduct), $(NewValueList)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error."
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    EndWait
	    Debug-Output "Registry error: add value list."
	    CloseRegKey $(KeyProduct)
	    CloseRegKey $(SoftNetRulesKey)
	    goto fatalregistry
	endif

	set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareType)},+
			    {use,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareUse)}, +
			    {bindform,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareBindForm)}, +
			    {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareClass)}, +
			    {bindable,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareBindable)}, +
			    {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}, +
			    {Infname ,$(NoTitle),$(!REG_VT_SZ),$(STF_CONTEXTINFNAME)} }

	Shell  $(UtilityInf), AddValueList, $(SoftNetRulesKey), $(NewValueList)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error."
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	CloseRegKey $(KeyProduct)
	CloseRegKey $(SoftNetRulesKey)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    EndWait
	    Debug-Output "Resgitry error: add value list."
	    goto fatalregistry
	endif
    endif

;
;   Create the HARDWARE\Netcard region and its corresponding service
;
    Shell $(UtilityInf), AddHardwareComponent, $(ProductHardwareName),$(STF_CONTEXTINFNAME),$(ProductKeyName)

    ifint $($R4) != -1
	Set OEM_ABANDON_OPTIONS = >($(OEM_ABANDON_OPTIONS), $(!NTN_SoftwareBase)"\Microsoft\Windows NT\CurrentVersion\NetworkCards\"$($R4))
    endif
		
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "Cannot add hardware component"
	goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	EndWait
	Debug-Output "Registry error: add hardware component"
	CloseRegKey $($R1)
	CloseRegKey $($R2)
	CloseRegKey $($R3)
	goto fatalregistry
    endif

;
;   At this point:
;     $R1  Registry key variable for HARDWARE\Netcard\(n)
;     $R2  Registry key variable for HARDWARE\Netcard\(n)\\NetRules
;     $R3  Registry key handle for <service>\Parameters key
;     $R4  Adapter number assigned to adapter
;     $R5  Service name generated by combining svc name with adapter number
;
    set KeyParameters = $($R3)
    set KeyAdapterRules = $($R2)
    set AdapterNumber = $($R4)

    set NewValueList = {{Manufacturer,$(NoTitle),$(!REG_VT_SZ),$(Manufacturer)},+
		       {Title,$(NoTitle),$(!REG_VT_SZ),"["$($R4)"] "$(ProductHardware$(Option)Title)},+
		       {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductHardware$(Option)Description)},+
		       {ProductName,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareName)},+
		       {ServiceName,$(NoTitle),$(!REG_VT_SZ),$($R5)},+
		       {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}

    Shell  $(UtilityInf), AddValueList, $($R1), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error"
	goto ShellCodeError
    endif

    CloseRegKey $($R1)

    set TempProdName = """"$(ProductHardwareName)$(AdapterNumber)""""
    set TempBindForm = $(TempProdName)$(NetRuleHardwareBindForm)

    set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleHardwareType)},+
			{bindform,$(NoTitle),$(!REG_VT_SZ),$(TempBindForm)}, +
			{class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleHardwareClass)}, +
			{InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}, +
			{Infname ,$(NoTitle),$(!REG_VT_SZ),$(STF_CONTEXTINFNAME)}}

    Shell  $(UtilityInf), AddValueList, $(KeyAdapterRules), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error."
	goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	EndWait
	Debug-Output "Resgitry error: add value list."
	CloseRegKey $(KeyParameters)
	CloseRegKey $(KeyAdapterRules)
	goto fatalregistry
    endif

    CloseRegKey $(KeyAdapterRules)

    goto writeparameters
;
;   REQUIRED:   $(KeyParameters) contains service Parameters key handle
;
writeparameters = +

    Shell $(UtilityInf), GetBusTypeDialog, $(ProductHardware$(Option)Description)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error."
	goto ShellCodeError
    endif

    ifstr(i) $($R0) == ERROR
        Debug-Output "GetBusTypeDialog error."

        Shell $(UtilityInf), GetBusTypeNum

        ifint $($ShellCode) != $(!SHELL_CODE_OK)
            Debug-Output "ShellCode error."
            goto ShellCodeError
        endif

        set BusTypeNum = $($R1)
        set BusNumber  = 0
    else
        set BusTypeNum = $($R1)
        set BusNumber  = $($R2)
    endif


;
;   Add the rest of the parameters to the Services area
;

    ifstr $(Option) == MDGISA

	set DMAChannelValue = *($(DMAChannelValues), ~($(DMAChannelList),$(DMAChannelIndex)))

	set IRQValue = *($(IRQValues), ~($(IRQList),$(IRQValueIndex)))

	set IOLocationValue = *($(IOLocationValues), ~($(IOLocationList),$(IOLocationIndex)))

	set NewValueList = {{InterruptNumber,$(NoTitle),$(!REG_VT_DWORD),$(IRQValue)},+
			{BusType,        $(NoTitle),$(!REG_VT_DWORD),$(BusTypeNum)},+
			{BusNumber,      $(NoTitle),$(!REG_VT_DWORD),$(BusNumber)},+
			{MediaType,      $(NoTitle),$(!REG_VT_DWORD),2},+
			{IoLocation,     $(NoTitle),$(!REG_VT_DWORD),$(IOLocationValue)},+
			{DmaChannel,     $(NoTitle),$(!REG_VT_DWORD),$(DMAChannelValue)},+
			{MaxFrameSize,   $(NoTitle),$(!REG_VT_DWORD),$(MaxFrameSize)}}
    else
	set NewValueList = {+
			{BusType,        $(NoTitle),$(!REG_VT_DWORD),$(BusTypeNum)},+
			{BusNumber,      $(NoTitle),$(!REG_VT_DWORD),$(BusNumber)},+
			{MediaType,      $(NoTitle),$(!REG_VT_DWORD),2},+
			{$(McaEisaKeyword), $(NoTitle), $(!REG_VT_DWORD), $(McaEisaId)},+
			{SlotNumber,     $(NoTitle),$(!REG_VT_DWORD),$(SlotNumber)},+
			{MaxFrameSize,   $(NoTitle),$(!REG_VT_DWORD),$(MaxFrameSize)}}
    endif
    
    ifstr $(LAA) != ""
	; Add the LAA to the end of the value list

	set NewValueList = >($(NewValueList),+
			     {NetworkAddress, $(NoTitle), $(!REG_VT_SZ), $(LAA)})
    endif

    Shell  $(UtilityInf), AddValueList, $(KeyParameters), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error."
	goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	Debug-Output "Registry error: Add value list"
	CloseRegKey $(KeyParameters)
	goto fatalregistry
    endif

    ifstr $(oldLAA) != ""
	ifstr $(LAA) == ""
	    ; The old LAA has been cleared, so delete the key from registry
	    
	    DeleteRegValue $(KeyParameters) NetworkAddress
	endif
    endif

    CloseRegKey $(KeyParameters)

    EndWait

    goto successful

;-----------------------------------------------
; Binding section
;-----------------------------------------------
bindingadapter =+
    set Error = "Binding: Sorry, not yet implemented."
    goto fatal

;-----------------------------------------------
; Removeadapter section
;-----------------------------------------------

removeadapter = +
    Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
	; Remove Software Component
	Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    else
	Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), $(!NTN_RegBase)     
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    endif

    goto end

;-----------------------------------------------
; Upgrade Software section
;-----------------------------------------------

UpgradeSoftware = +
    ;
    ; First determine whether we want to do upgrade or update for software
    ; or hardware component. Then we will determine whether the Mode is
    ; update or upgrade.
    ;
    ; If the same version of the product existed in the registry, we do
    ; update. Otherwise, we will do a upgrade
    ;
    ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
	; Upgrade software component
	;
	; see whether the same version exist or not
	;
	OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct

	Ifstr $(KeyProduct) != $(KeyNull)
	    GetRegValue $(KeyProduct),"MajorVersion", VersionInfo
	    set Version = *($(VersionInfo), 4)

	    ;
	    ; Update the binaries
	    ;
	    shell $(UtilityInf) GetInfFileNameFromRegistry $(KeyProduct)
	    ifint $($ShellCode) != $(!SHELL_CODE_OK)
		goto ShellCodeError
	    endif

	    set !UG_Filename = $($R0)

	    ; Split-String $(!NTN_Infname), "\", FilenameList
	    ; QueryListSize ListSize $(FilenameList)
	    ; set !UG_Filename = *($(FilenameList), $(ListSize))

	    ifstr(i) $(!UG_Filename) != ""
		install "Install-Update"
		ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
		    goto fatal
		endif
	    endif

	    ; Upgrade the version number
	    ;
	    SetRegValue $(KeyProduct) {MajorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMajorVersion)}
	    SetRegValue $(KeyProduct) {MinorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMinorVersion)}

	    ;
	    ; do nothing for update
	    ;
	    ifint $(Version) != $(ProductMajorVersion)
	       ;
	       ; If the major version number is not the same,
	       ; it is major upgrade. So let Upgrade the product
	       ;
	       ;
	       ; make other upgrade change if necessary
	       ;
	    endif
	    CloseRegKey $(KeyProduct)
	else
	    ;
	    ; Cannot Open software key, goto ERROR
	    ;
	    goto fatalregistry
	endif
    else
	;
	; upgrade/update hardware component
	; There is no different between upgrade and update for hardware
	; component
	;
	; 1. Get the Service Name
	; 2. Change the NetRule section if necessary
	;
	OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) +
	      $(MAXIMUM_ALLOWED) NetworkCardKey
	Ifstr(i) $(NetworkCardKey) != $(KeyNull)
	    ;
	    ; Get Service name
	    ;
	    GetRegValue $(NetworkCardKey),"ServiceName", ServiceNameInfo
	    set ServiceName = *($(ServiceNameInfo), 4)
	
	    ;
	    ; Change the NetRule if necessary
	    ;
	    OpenRegKey $(NetworkCardKey) "" "NetRules" +
		$(MAXIMUM_ALLOWED) NetRuleKey
	    Ifstr(i) $(NetRuleKey) != $(KeyNull)
		;
		; Make the change....
		;
	    else
		;
		; Error, cannot open net rules key
		;
		CloseRegKey $(NetworkCardKey)
		goto fatalregistry
	    endif

	    CloseRegKey $(NetRuleKey)
	    CloseRegKey $(NetworkCardKey)
	else
	    ;
	    ; Error, cannot open network card key
	    ;
	    goto fatalregistry
	endif
	;
	; 3. Change the service section of the hardware. i.e.,
	;    ParameterName change, value change, etc.
	;
	OpenRegKey $(!REG_H_LOCAL) "" +
	      $(!NTN_ServiceBase)"\"$(ServiceName) +
	      $(MAXIMUM_ALLOWED) ServiceKey

	Ifstr(i) $(ServiceKey) != $(KeyNull)
	    ;
	    ; Get the ServiceKey to change the Start value
	    ; or Type value. Or open Parameters key to
	    ; change the hardware parameters if necessary.
	    ;
	    CloseRegKey $(ServiceKey)
	else
	    ;
	    ; Error, cannot open network card key
	    ;
	    goto fatalregistry
	endif
    endif
										
    goto end
    ;
    ; End of Upgrade Software
    ;

;****************************************************************************
;
;  Escape hatches
;

successful = +
    goto end

abandon = +
    ForListDo $(OEM_ABANDON_OPTIONS)
	Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), $($)        
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    EndForListDo

    Ifstr(i) $(OEM_ABANDON_SOFTWARE) == TRUE
	; Remove Software Component
	Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), FALSE
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    endif

    goto end

;
; warning display
;
warning = +
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "WARNING", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
	goto $(to)
    else-ifstr(i) $($R1) == "CANCEL"
	goto $(from)
    else
	goto "end"
    endif


;
; non fatal error display
;
nonfatalinfo = +
    set Severity = STATUS
    set CommonStatus = STATUS_USERCANCEL
    goto nonfatalmsg

nonfatal = +
    set Severity = NONFATAL
    goto nonfatalmsg

nonfatalmsg = +
    ifstr(i) $(Error) == ""
	set Severity = NONFATAL
	Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    goto ShellCodeError
	endif
	set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "NONFATAL", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
	goto $(from)
    else
	goto "end"
    endif

;
;  Registry is broken
;
fatalregistry = +
    Shell $(UtilityInf) RegistryErrorString $(RegistryErrorIndex)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    set Error = $($R0)
    goto fatal
;
; fatal error display
;
fatal = +
    ifstr(i) $(Error) == ""
	Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    goto ShellCodeError
	endif
	set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "FATAL", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif

    goto setfailed

;
;  Shelling error
;
ShellCodeError = +
    set DlgType      = "MessageBox"
    set STF_MB_TITLE = $(ShellCodeErrorTitle)
    set STF_MB_TEXT  = $(ShellCodeErrorText)
    set STF_MB_TYPE  = 1
    set STF_MB_ICON  = 3
    set STF_MB_DEF   = 1
    ui start "Error Message"
    goto setfailed

setfailed = +
    set CommonStatus = STATUS_FAILED
    ;
    ; if OEM_ABANDON_ON == TRUE, then remove the registry entries
    ;
    ifstr(i) $(OEM_ABANDON_ON) == TRUE
	set OEM_ABANDON_ON = FALSE
	goto abandon
    endif
    goto end

end = +
    goto term

term = +

    Return $(CommonStatus)

;***************************************************************
;  INSTALL SECTIONS
;***************************************************************

[Install-Driver]
    set STF_VITAL = ""

    ifstr(i) $(AddCopy) == "YES"

	;
	; Add the files to the copy list
	;
	AddSectionFilesToCopyList Files-Driver $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers

    endif

    ifstr(i) $(DoCopy) == "YES"

       ;
       ; Copy files in the copy list
       ;
       set !STF_NCPA_FLUSH_COPYLIST = TRUE
       CopyFilesInCopyList

    endif

    Exit

[Install-Update]
   set STF_VITAL        = ""
   set STF_OVERWRITE    = "VERIFYSOURCEOLDER"
   ;set STF_VERSION     = "YES"

   AddSectionFilesToCopyList Files-Driver $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers
   AddSectionFilesToCopyList Files-Inf $(SrcDir) $(!STF_WINDOWSSYSPATH)

   set !STF_NCPA_FLUSH_COPYLIST = TRUE
   CopyFilesInCopyList

   exit


[Install-Dll]
   set STF_VITAL        = ""

   ifstr(i) $(AddCopy) == "YES"
       AddSectionFilesToCopyList Files-Dll $(SrcDir) $(!STF_WINDOWSSYSPATH)
   endif

   ifstr(i) $(DoCopy) == "YES"
       set !STF_NCPA_FLUSH_COPYLIST = TRUE
       CopyFilesInCopyList
   endif

   exit


[Source Media Descriptions]
    1  = "Madge Driver Disk"  , TAGFILE = disk2
    2  = "Windows NT Setup CD-ROM Disk"  , TAGFILE = disk2

[ProductType]
STF_PRODUCT  = Winnt
STF_PLATFORM = I386

[Files-Inf]
1, oemsetup.inf, SIZE=999, RENAME=$(!UG_Filename)

[Files-Driver]
1, smartnt.sys , SIZE=999

[Files-Dll]
1, madgedlg.dll, SIZE=999
1, madgedlg.hlp, SIZE=999
