The Compaq AVGA driver is provided to support Compaq machines with
this controller built-in.  The following video modes are supported:

    640x480, 16 colors
    640x480, 256 colors (requires 512kb video RAM)
    800x600, 256 colors (requires 512kb video RAM and external monitor) 

To create an install disk for this driver:

1.  Boot MS-DOS

2.  Copy the contents of this directory to a floppy in A:

3.  Copy the compressed VGA.DL_ and VGA256.DL_ from \I386 to a
    temporary directory (these files are also found on disks 6 and 7
    of the x86 floppy install set)

4.  Run the following commands:

        EXPAND VGA.DL_ A:\VGA.DLL
        EXPAND VGA256.DL_ A:\VGA256.DLL

The driver can then be installed during the text-mode portion of
Setup, or using maintenance mode Setup once Windows NT is running.


